(footprint "QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/8008S.pdf#page=16), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.6 -0.6)
		(size 0.97 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.6 0.6)
		(size 0.97 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.6 -0.6)
		(size 0.97 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.6 0.6)
		(size 0.97 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd custom
		(at -1.95 -1.35)
		(size 0.179289 0.179289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3375 -0.0625)
					(xy 0.274112 -0.0625)
					(xy 0.3375 0.000888)
					(xy 0.3375 0.0625)
					(xy -0.3375 0.0625)
				)
				(width 0.125)
			)
		)
	)
	(pad "2" smd roundrect
		(at -1.95 -0.9)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.95 -0.45)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.95 0)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.95 0.45)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.95 0.9)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd custom
		(at -1.95 1.35)
		(size 0.179289 0.179289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3375 -0.0625)
					(xy 0.3375 -0.0625)
					(xy 0.3375 -0.000888)
					(xy 0.274112 0.0625)
					(xy -0.3375 0.0625)
				)
				(width 0.125)
			)
		)
	)
	(pad "8" smd custom
		(at -1.35 1.95)
		(size 0.179289 0.179289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.0625 -0.274112)
					(xy 0.000888 -0.3375)
					(xy 0.0625 -0.3375)
					(xy 0.0625 0.3375)
					(xy -0.0625 0.3375)
				)
				(width 0.125)
			)
		)
	)
	(pad "9" smd roundrect
		(at -0.9 1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.45 1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0.45 1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.9 1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd custom
		(at 1.35 1.95)
		(size 0.179289 0.179289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.0625 -0.3375)
					(xy -0.000888 -0.3375)
					(xy 0.0625 -0.274112)
					(xy 0.0625 0.3375)
					(xy -0.0625 0.3375)
				)
				(width 0.125)
			)
		)
	)
	(pad "15" smd custom
		(at 1.95 1.35)
		(size 0.179289 0.179289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3375 -0.0625)
					(xy 0.3375 -0.0625)
					(xy 0.3375 0.0625)
					(xy -0.274112 0.0625)
					(xy -0.3375 -0.000888)
				)
				(width 0.125)
			)
		)
	)
	(pad "16" smd roundrect
		(at 1.95 0.9)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.95 0.45)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.95 0)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.95 -0.45)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.95 -0.9)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd custom
		(at 1.95 -1.35)
		(size 0.179289 0.179289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3375 0.000888)
					(xy -0.274112 -0.0625)
					(xy 0.3375 -0.0625)
					(xy 0.3375 0.0625)
					(xy -0.3375 0.0625)
				)
				(width 0.125)
			)
		)
	)
	(pad "22" smd custom
		(at 1.35 -1.95)
		(size 0.179289 0.179289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.0625 -0.3375)
					(xy 0.0625 -0.3375)
					(xy 0.0625 0.274112)
					(xy -0.000888 0.3375)
					(xy -0.0625 0.3375)
				)
				(width 0.125)
			)
		)
	)
	(pad "23" smd roundrect
		(at 0.9 -1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 0.45 -1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 0 -1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -0.45 -1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -0.9 -1.95)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd custom
		(at -1.35 -1.95)
		(size 0.179289 0.179289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.0625 -0.3375)
					(xy 0.0625 -0.3375)
					(xy 0.0625 0.3375)
					(xy 0.000888 0.3375)
					(xy -0.0625 0.274112)
				)
				(width 0.125)
			)
		)
	)
	(pad "29" smd rect
		(at 0 0)
		(size 2.4 2.4)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
