(footprint "QFN-28-1EP_5x5mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 28 Pin (JEDEC MO-220-K.01, variation VHHD-1,  https://www.jedec.org/system/files/docs/MO-220K01.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-28-1EP_5x5mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
		(at 0 3.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.125 -1.125)
		(size 0.17446 0.17446)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.133177 -0.133177)
					(xy 0.133177 -0.133177)
					(xy 0.133177 -0.104929)
					(xy -0.104929 0.133177)
					(xy -0.133177 0.133177)
				)
				(width 0.096447)
			)
		)
	)
	(pad "" smd custom
		(at -1.125 -0.45)
		(size 0.205289 0.205289)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.111378 -0.292779)
					(xy -0.070359 -0.292779)
					(xy 0.111378 -0.111041)
					(xy 0.111378 0.111041)
					(xy -0.070359 0.292779)
					(xy -0.111378 0.292779)
				)
				(width 0.140046)
			)
		)
	)
	(pad "" smd custom
		(at -1.125 0.45)
		(size 0.205289 0.205289)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.111378 -0.292779)
					(xy -0.070359 -0.292779)
					(xy 0.111378 -0.111041)
					(xy 0.111378 0.111041)
					(xy -0.070359 0.292779)
					(xy -0.111378 0.292779)
				)
				(width 0.140046)
			)
		)
	)
	(pad "" smd custom
		(at -1.125 1.125)
		(size 0.17446 0.17446)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.133177 -0.133177)
					(xy -0.104929 -0.133177)
					(xy 0.133177 0.104929)
					(xy 0.133177 0.133177)
					(xy -0.133177 0.133177)
				)
				(width 0.096447)
			)
		)
	)
	(pad "" smd custom
		(at -0.45 -1.125)
		(size 0.205289 0.205289)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.292779 -0.111378)
					(xy 0.292779 -0.111378)
					(xy 0.292779 -0.070359)
					(xy 0.111041 0.111378)
					(xy -0.111041 0.111378)
					(xy -0.292779 -0.070359)
				)
				(width 0.140046)
			)
		)
	)
	(pad "" smd custom
		(at -0.45 -0.45)
		(size 0.59892 0.59892)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236119 -0.131171)
					(xy -0.131171 -0.236119)
					(xy 0.131171 -0.236119)
					(xy 0.236119 -0.131171)
					(xy 0.236119 0.131171)
					(xy 0.131171 0.236119)
					(xy -0.131171 0.236119)
					(xy -0.236119 0.131171)
				)
				(width 0.253366)
			)
		)
	)
	(pad "" smd custom
		(at -0.45 0.45)
		(size 0.59892 0.59892)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236119 -0.131171)
					(xy -0.131171 -0.236119)
					(xy 0.131171 -0.236119)
					(xy 0.236119 -0.131171)
					(xy 0.236119 0.131171)
					(xy 0.131171 0.236119)
					(xy -0.131171 0.236119)
					(xy -0.236119 0.131171)
				)
				(width 0.253366)
			)
		)
	)
	(pad "" smd custom
		(at -0.45 1.125)
		(size 0.205289 0.205289)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.292779 0.070359)
					(xy -0.111041 -0.111378)
					(xy 0.111041 -0.111378)
					(xy 0.292779 0.070359)
					(xy 0.292779 0.111378)
					(xy -0.292779 0.111378)
				)
				(width 0.140046)
			)
		)
	)
	(pad "" smd custom
		(at 0.45 -1.125)
		(size 0.205289 0.205289)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.292779 -0.111378)
					(xy 0.292779 -0.111378)
					(xy 0.292779 -0.070359)
					(xy 0.111041 0.111378)
					(xy -0.111041 0.111378)
					(xy -0.292779 -0.070359)
				)
				(width 0.140046)
			)
		)
	)
	(pad "" smd custom
		(at 0.45 -0.45)
		(size 0.59892 0.59892)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236119 -0.131171)
					(xy -0.131171 -0.236119)
					(xy 0.131171 -0.236119)
					(xy 0.236119 -0.131171)
					(xy 0.236119 0.131171)
					(xy 0.131171 0.236119)
					(xy -0.131171 0.236119)
					(xy -0.236119 0.131171)
				)
				(width 0.253366)
			)
		)
	)
	(pad "" smd custom
		(at 0.45 0.45)
		(size 0.59892 0.59892)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236119 -0.131171)
					(xy -0.131171 -0.236119)
					(xy 0.131171 -0.236119)
					(xy 0.236119 -0.131171)
					(xy 0.236119 0.131171)
					(xy 0.131171 0.236119)
					(xy -0.131171 0.236119)
					(xy -0.236119 0.131171)
				)
				(width 0.253366)
			)
		)
	)
	(pad "" smd custom
		(at 0.45 1.125)
		(size 0.205289 0.205289)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.292779 0.070359)
					(xy -0.111041 -0.111378)
					(xy 0.111041 -0.111378)
					(xy 0.292779 0.070359)
					(xy 0.292779 0.111378)
					(xy -0.292779 0.111378)
				)
				(width 0.140046)
			)
		)
	)
	(pad "" smd custom
		(at 1.125 -1.125)
		(size 0.17446 0.17446)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.133177 -0.133177)
					(xy 0.133177 -0.133177)
					(xy 0.133177 0.133177)
					(xy 0.104929 0.133177)
					(xy -0.133177 -0.104929)
				)
				(width 0.096447)
			)
		)
	)
	(pad "" smd custom
		(at 1.125 -0.45)
		(size 0.205289 0.205289)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.111378 -0.111041)
					(xy 0.070359 -0.292779)
					(xy 0.111378 -0.292779)
					(xy 0.111378 0.292779)
					(xy 0.070359 0.292779)
					(xy -0.111378 0.111041)
				)
				(width 0.140046)
			)
		)
	)
	(pad "" smd custom
		(at 1.125 0.45)
		(size 0.205289 0.205289)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.111378 -0.111041)
					(xy 0.070359 -0.292779)
					(xy 0.111378 -0.292779)
					(xy 0.111378 0.292779)
					(xy 0.070359 0.292779)
					(xy -0.111378 0.111041)
				)
				(width 0.140046)
			)
		)
	)
	(pad "" smd custom
		(at 1.125 1.125)
		(size 0.17446 0.17446)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.133177 0.104929)
					(xy 0.104929 -0.133177)
					(xy 0.133177 -0.133177)
					(xy 0.133177 0.133177)
					(xy -0.133177 0.133177)
				)
				(width 0.096447)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.3125 -1.5)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.3125 -1)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.3125 -0.5)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.3125 0)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.3125 0.5)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.3125 1)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.3125 1.5)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -1.5 2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -1 2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.5 2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0.5 2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1 2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.5 2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 2.3125 1.5)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.3125 1)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 2.3125 0.5)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 2.3125 0)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 2.3125 -0.5)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.3125 -1)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.3125 -1.5)
		(size 1.075 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.5 -2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1 -2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 0.5 -2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 0 -2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -0.5 -2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -1 -2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -1.5 -2.3125)
		(size 0.25 1.075)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" thru_hole circle
		(at -0.9 -0.9)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -0.9 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -0.9 0.9)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0 -0.9)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" smd rect
		(at 0 0)
		(size 2.3 2.3)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "29" smd rect
		(at 0 0)
		(size 2.7 2.7)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "29" thru_hole circle
		(at 0 0.9)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0.9 -0.9)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0.9 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0.9 0.9)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP2.7x2.7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
