(footprint "QFN-28-1EP_5x5mm_P0.5mm_EP3.1x3.1mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 28 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/TMC2202_TMC2208_TMC2224_datasheet_rev1.14.pdf#page=77), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-28-1EP_5x5mm_P0.5mm_EP3.1x3.1mm_ThermalVias"
		(at 0 3.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.3 -1.3)
		(size 0.271622 0.271622)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.100778)
					(xy 0.100778 -0.100778)
					(xy 0.100778 -0.026143)
					(xy -0.026143 0.100778)
					(xy -0.100778 0.100778)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at -1.3 -0.7)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.181401)
					(xy -0.006765 -0.181401)
					(xy 0.100778 -0.073857)
					(xy 0.100778 0.073857)
					(xy -0.006765 0.181401)
					(xy -0.100778 0.181401)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at -1.3 0)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.181401)
					(xy -0.006765 -0.181401)
					(xy 0.100778 -0.073857)
					(xy 0.100778 0.073857)
					(xy -0.006765 0.181401)
					(xy -0.100778 0.181401)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at -1.3 0.7)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.181401)
					(xy -0.006765 -0.181401)
					(xy 0.100778 -0.073857)
					(xy 0.100778 0.073857)
					(xy -0.006765 0.181401)
					(xy -0.100778 0.181401)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at -1.3 1.3)
		(size 0.271622 0.271622)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.100778)
					(xy -0.026143 -0.100778)
					(xy 0.100778 0.026143)
					(xy 0.100778 0.100778)
					(xy -0.100778 0.100778)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at -0.7 -1.3)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.181401 -0.100778)
					(xy 0.181401 -0.100778)
					(xy 0.181401 -0.006765)
					(xy 0.073857 0.100778)
					(xy -0.073857 0.100778)
					(xy -0.181401 -0.006765)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at -0.7 -0.7)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at -0.7 0)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at -0.7 0.7)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at -0.7 1.3)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.181401 0.006765)
					(xy -0.073857 -0.100778)
					(xy 0.073857 -0.100778)
					(xy 0.181401 0.006765)
					(xy 0.181401 0.100778)
					(xy -0.181401 0.100778)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 0 -1.3)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.181401 -0.100778)
					(xy 0.181401 -0.100778)
					(xy 0.181401 -0.006765)
					(xy 0.073857 0.100778)
					(xy -0.073857 0.100778)
					(xy -0.181401 -0.006765)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 0 -0.7)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at 0 0)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at 0 0.7)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at 0 1.3)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.181401 0.006765)
					(xy -0.073857 -0.100778)
					(xy 0.073857 -0.100778)
					(xy 0.181401 0.006765)
					(xy 0.181401 0.100778)
					(xy -0.181401 0.100778)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 0.7 -1.3)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.181401 -0.100778)
					(xy 0.181401 -0.100778)
					(xy 0.181401 -0.006765)
					(xy 0.073857 0.100778)
					(xy -0.073857 0.100778)
					(xy -0.181401 -0.006765)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 0.7 -0.7)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at 0.7 0)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at 0.7 0.7)
		(size 0.460271 0.460271)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178092 -0.091864)
					(xy -0.091864 -0.178092)
					(xy 0.091864 -0.178092)
					(xy 0.178092 -0.091864)
					(xy 0.178092 0.091864)
					(xy 0.091864 0.178092)
					(xy -0.091864 0.178092)
					(xy -0.178092 0.091864)
				)
				(width 0.208173)
			)
		)
	)
	(pad "" smd custom
		(at 0.7 1.3)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.181401 0.006765)
					(xy -0.073857 -0.100778)
					(xy 0.073857 -0.100778)
					(xy 0.181401 0.006765)
					(xy 0.181401 0.100778)
					(xy -0.181401 0.100778)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 1.3 -1.3)
		(size 0.271622 0.271622)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.100778)
					(xy 0.100778 -0.100778)
					(xy 0.100778 0.100778)
					(xy 0.026143 0.100778)
					(xy -0.100778 -0.026143)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 1.3 -0.7)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.073857)
					(xy 0.006765 -0.181401)
					(xy 0.100778 -0.181401)
					(xy 0.100778 0.181401)
					(xy 0.006765 0.181401)
					(xy -0.100778 0.073857)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 1.3 0)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.073857)
					(xy 0.006765 -0.181401)
					(xy 0.100778 -0.181401)
					(xy 0.100778 0.181401)
					(xy 0.006765 0.181401)
					(xy -0.100778 0.073857)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 1.3 0.7)
		(size 0.285324 0.285324)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 -0.073857)
					(xy 0.006765 -0.181401)
					(xy 0.100778 -0.181401)
					(xy 0.100778 0.181401)
					(xy 0.006765 0.181401)
					(xy -0.100778 0.073857)
				)
				(width 0.201556)
			)
		)
	)
	(pad "" smd custom
		(at 1.3 1.3)
		(size 0.271622 0.271622)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.100778 0.026143)
					(xy 0.026143 -0.100778)
					(xy 0.100778 -0.100778)
					(xy 0.100778 0.100778)
					(xy -0.100778 0.100778)
				)
				(width 0.201556)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.375 -1.5)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.375 -1)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.375 -0.5)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.375 0)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.375 0.5)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.375 1)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.375 1.5)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -1.5 2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -1 2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.5 2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0.5 2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1 2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.5 2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 2.375 1.5)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.375 1)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 2.375 0.5)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 2.375 0)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 2.375 -0.5)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.375 -1)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.375 -1.5)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.5 -2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1 -2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 0.5 -2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 0 -2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -0.5 -2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -1 -2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -1.5 -2.375)
		(size 0.25 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" thru_hole circle
		(at -1.05 -1.05)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -1.05 -0.35)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -1.05 0.35)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -1.05 1.05)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -0.35 -1.05)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -0.35 -0.35)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -0.35 0.35)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -0.35 1.05)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" smd rect
		(at 0 0)
		(size 2.6 2.6)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "29" smd rect
		(at 0 0)
		(size 3.1 3.1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "29" thru_hole circle
		(at 0.35 -1.05)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0.35 -0.35)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0.35 0.35)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0.35 1.05)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 1.05 -1.05)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 1.05 -0.35)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 1.05 0.35)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 1.05 1.05)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP3.1x3.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
