(footprint "QFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 28 Pin (https://www.silabs.com/documents/public/data-sheets/C8051F32x.pdf#page=39), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.81 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm_ThermalVias"
		(at 0 3.81 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.3125 -1.3125)
		(size 0.341781 0.341781)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127896 -0.127896)
					(xy 0.127896 -0.127896)
					(xy 0.127896 -0.037322)
					(xy -0.037322 0.127896)
					(xy -0.127896 0.127896)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at -1.3125 -0.5)
		(size 0.36584 0.36584)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127896 -0.281372)
					(xy -0.003297 -0.281372)
					(xy 0.127896 -0.150178)
					(xy 0.127896 0.150178)
					(xy -0.003297 0.281372)
					(xy -0.127896 0.281372)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at -1.3125 0.5)
		(size 0.36584 0.36584)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127896 -0.281372)
					(xy -0.003297 -0.281372)
					(xy 0.127896 -0.150178)
					(xy 0.127896 0.150178)
					(xy -0.003297 0.281372)
					(xy -0.127896 0.281372)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at -1.3125 1.3125)
		(size 0.341781 0.341781)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127896 -0.127896)
					(xy -0.037322 -0.127896)
					(xy 0.127896 0.037322)
					(xy 0.127896 0.127896)
					(xy -0.127896 0.127896)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 -1.3125)
		(size 0.36584 0.36584)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.281372 -0.127896)
					(xy 0.281372 -0.127896)
					(xy 0.281372 -0.003297)
					(xy 0.150178 0.127896)
					(xy -0.150178 0.127896)
					(xy -0.281372 -0.003297)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 -0.5)
		(size 0.69685 0.69685)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.287583 -0.186775)
					(xy -0.186775 -0.287583)
					(xy 0.186775 -0.287583)
					(xy 0.287583 -0.186775)
					(xy 0.287583 0.186775)
					(xy 0.186775 0.287583)
					(xy -0.186775 0.287583)
					(xy -0.287583 0.186775)
				)
				(width 0.24337)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 0.5)
		(size 0.69685 0.69685)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.287583 -0.186775)
					(xy -0.186775 -0.287583)
					(xy 0.186775 -0.287583)
					(xy 0.287583 -0.186775)
					(xy 0.287583 0.186775)
					(xy 0.186775 0.287583)
					(xy -0.186775 0.287583)
					(xy -0.287583 0.186775)
				)
				(width 0.24337)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 1.3125)
		(size 0.36584 0.36584)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.281372 0.003297)
					(xy -0.150178 -0.127896)
					(xy 0.150178 -0.127896)
					(xy 0.281372 0.003297)
					(xy 0.281372 0.127896)
					(xy -0.281372 0.127896)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 -1.3125)
		(size 0.36584 0.36584)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.281372 -0.127896)
					(xy 0.281372 -0.127896)
					(xy 0.281372 -0.003297)
					(xy 0.150178 0.127896)
					(xy -0.150178 0.127896)
					(xy -0.281372 -0.003297)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 -0.5)
		(size 0.69685 0.69685)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.287583 -0.186775)
					(xy -0.186775 -0.287583)
					(xy 0.186775 -0.287583)
					(xy 0.287583 -0.186775)
					(xy 0.287583 0.186775)
					(xy 0.186775 0.287583)
					(xy -0.186775 0.287583)
					(xy -0.287583 0.186775)
				)
				(width 0.24337)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 0.5)
		(size 0.69685 0.69685)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.287583 -0.186775)
					(xy -0.186775 -0.287583)
					(xy 0.186775 -0.287583)
					(xy 0.287583 -0.186775)
					(xy 0.287583 0.186775)
					(xy 0.186775 0.287583)
					(xy -0.186775 0.287583)
					(xy -0.287583 0.186775)
				)
				(width 0.24337)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 1.3125)
		(size 0.36584 0.36584)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.281372 0.003297)
					(xy -0.150178 -0.127896)
					(xy 0.150178 -0.127896)
					(xy 0.281372 0.003297)
					(xy 0.281372 0.127896)
					(xy -0.281372 0.127896)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at 1.3125 -1.3125)
		(size 0.341781 0.341781)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127896 -0.127896)
					(xy 0.127896 -0.127896)
					(xy 0.127896 0.127896)
					(xy 0.037322 0.127896)
					(xy -0.127896 -0.037322)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at 1.3125 -0.5)
		(size 0.36584 0.36584)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127896 -0.150178)
					(xy 0.003297 -0.281372)
					(xy 0.127896 -0.281372)
					(xy 0.127896 0.281372)
					(xy 0.003297 0.281372)
					(xy -0.127896 0.150178)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at 1.3125 0.5)
		(size 0.36584 0.36584)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127896 -0.150178)
					(xy 0.003297 -0.281372)
					(xy 0.127896 -0.281372)
					(xy 0.127896 0.281372)
					(xy 0.003297 0.281372)
					(xy -0.127896 0.150178)
				)
				(width 0.255792)
			)
		)
	)
	(pad "" smd custom
		(at 1.3125 1.3125)
		(size 0.341781 0.341781)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127896 0.037322)
					(xy 0.037322 -0.127896)
					(xy 0.127896 -0.127896)
					(xy 0.127896 0.127896)
					(xy -0.127896 0.127896)
				)
				(width 0.255792)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.4 -1.5)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.4 -1)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.4 -0.5)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.4 0)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.4 0.5)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.4 1)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.4 1.5)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -1.5 2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -1 2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.5 2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0.5 2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1 2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.5 2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 2.4 1.5)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.4 1)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 2.4 0.5)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 2.4 0)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 2.4 -0.5)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.4 -1)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.4 -1.5)
		(size 0.9 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.5 -2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1 -2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 0.5 -2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 0 -2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -0.5 -2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -1 -2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -1.5 -2.4)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" thru_hole circle
		(at -1 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -1 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" smd rect
		(at 0 0)
		(size 2.5 2.5)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "29" smd rect
		(at 0 0)
		(size 3.25 3.25)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "29" thru_hole circle
		(at 0 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 1 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 1 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
