(footprint "QFN-28_4x4mm_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 28 Pin (http://www.st.com/resource/en/datasheet/stm32f031k6.pdf#page=90), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.33 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-28_4x4mm_P0.5mm"
		(at 0 3.33 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -1.9975 -1.5)
		(size 0.136863 0.136863)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3325 -0.08)
					(xy 0.19886 -0.08)
					(xy 0.3325 0.05364)
					(xy 0.3325 0.08)
					(xy -0.3325 0.08)
				)
				(width 0.09)
			)
		)
	)
	(pad "2" smd roundrect
		(at -1.9375 -1)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.9375 -0.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.9375 0)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.9375 0.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.9375 1)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd custom
		(at -1.9975 1.5)
		(size 0.136863 0.136863)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3325 -0.08)
					(xy 0.3325 -0.08)
					(xy 0.3325 -0.05364)
					(xy 0.19886 0.08)
					(xy -0.3325 0.08)
				)
				(width 0.09)
			)
		)
	)
	(pad "8" smd custom
		(at -1.5 1.9975)
		(size 0.136863 0.136863)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.08 -0.19886)
					(xy 0.05364 -0.3325)
					(xy 0.08 -0.3325)
					(xy 0.08 0.3325)
					(xy -0.08 0.3325)
				)
				(width 0.09)
			)
		)
	)
	(pad "9" smd roundrect
		(at -1 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.5 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0.5 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd custom
		(at 1.5 1.9975)
		(size 0.136863 0.136863)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.08 -0.3325)
					(xy -0.05364 -0.3325)
					(xy 0.08 -0.19886)
					(xy 0.08 0.3325)
					(xy -0.08 0.3325)
				)
				(width 0.09)
			)
		)
	)
	(pad "15" smd custom
		(at 1.9975 1.5)
		(size 0.136863 0.136863)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3325 -0.08)
					(xy 0.3325 -0.08)
					(xy 0.3325 0.08)
					(xy -0.19886 0.08)
					(xy -0.3325 -0.05364)
				)
				(width 0.09)
			)
		)
	)
	(pad "16" smd roundrect
		(at 1.9375 1)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.9375 0.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.9375 0)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.9375 -0.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.9375 -1)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd custom
		(at 1.9975 -1.5)
		(size 0.136863 0.136863)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3325 0.05364)
					(xy -0.19886 -0.08)
					(xy 0.3325 -0.08)
					(xy 0.3325 0.08)
					(xy -0.3325 0.08)
				)
				(width 0.09)
			)
		)
	)
	(pad "22" smd custom
		(at 1.5 -1.9975)
		(size 0.136863 0.136863)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.08 -0.3325)
					(xy 0.08 -0.3325)
					(xy 0.08 0.19886)
					(xy -0.05364 0.3325)
					(xy -0.08 0.3325)
				)
				(width 0.09)
			)
		)
	)
	(pad "23" smd roundrect
		(at 1 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 0.5 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 0 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -0.5 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -1 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd custom
		(at -1.5 -1.9975)
		(size 0.136863 0.136863)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.08 -0.3325)
					(xy 0.08 -0.3325)
					(xy 0.08 0.3325)
					(xy 0.05364 0.3325)
					(xy -0.08 0.19886)
				)
				(width 0.09)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28_4x4mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
