(footprint "QFN-32-1EP_4x4mm_P0.4mm_EP2.65x2.65mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 32 Pin (https://www.renesas.com/eu/en/package-image/pdf/outdrawing/l32.4x4a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-32-1EP_4x4mm_P0.4mm_EP2.65x2.65mm_ThermalVias"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.0875 -1.0875)
		(size 0.248041 0.248041)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.095739 -0.095739)
					(xy 0.095739 -0.095739)
					(xy 0.095739 -0.038978)
					(xy -0.038978 0.095739)
					(xy -0.095739 0.095739)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at -1.0875 -0.425)
		(size 0.273732 0.273732)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.095739 -0.246907)
					(xy -0.002645 -0.246907)
					(xy 0.095739 -0.148522)
					(xy 0.095739 0.148522)
					(xy -0.002645 0.246907)
					(xy -0.095739 0.246907)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at -1.0875 0.425)
		(size 0.273732 0.273732)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.095739 -0.246907)
					(xy -0.002645 -0.246907)
					(xy 0.095739 -0.148522)
					(xy 0.095739 0.148522)
					(xy -0.002645 0.246907)
					(xy -0.095739 0.246907)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at -1.0875 1.0875)
		(size 0.248041 0.248041)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.095739 -0.095739)
					(xy -0.038978 -0.095739)
					(xy 0.095739 0.038978)
					(xy 0.095739 0.095739)
					(xy -0.095739 0.095739)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at -0.425 -1.0875)
		(size 0.273732 0.273732)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.246907 -0.095739)
					(xy 0.246907 -0.095739)
					(xy 0.246907 -0.002645)
					(xy 0.148522 0.095739)
					(xy -0.148522 0.095739)
					(xy -0.246907 -0.002645)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at -0.425 -0.425)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at -0.425 0.425)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at -0.425 1.0875)
		(size 0.273732 0.273732)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.246907 0.002645)
					(xy -0.148522 -0.095739)
					(xy 0.148522 -0.095739)
					(xy 0.246907 0.002645)
					(xy 0.246907 0.095739)
					(xy -0.246907 0.095739)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at 0.425 -1.0875)
		(size 0.273732 0.273732)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.246907 -0.095739)
					(xy 0.246907 -0.095739)
					(xy 0.246907 -0.002645)
					(xy 0.148522 0.095739)
					(xy -0.148522 0.095739)
					(xy -0.246907 -0.002645)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at 0.425 -0.425)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at 0.425 0.425)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at 0.425 1.0875)
		(size 0.273732 0.273732)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.246907 0.002645)
					(xy -0.148522 -0.095739)
					(xy 0.148522 -0.095739)
					(xy 0.246907 0.002645)
					(xy 0.246907 0.095739)
					(xy -0.246907 0.095739)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at 1.0875 -1.0875)
		(size 0.248041 0.248041)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.095739 -0.095739)
					(xy 0.095739 -0.095739)
					(xy 0.095739 0.095739)
					(xy 0.038978 0.095739)
					(xy -0.095739 -0.038978)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at 1.0875 -0.425)
		(size 0.273732 0.273732)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.095739 -0.148522)
					(xy 0.002645 -0.246907)
					(xy 0.095739 -0.246907)
					(xy 0.095739 0.246907)
					(xy 0.002645 0.246907)
					(xy -0.095739 0.148522)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at 1.0875 0.425)
		(size 0.273732 0.273732)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.095739 -0.148522)
					(xy 0.002645 -0.246907)
					(xy 0.095739 -0.246907)
					(xy 0.095739 0.246907)
					(xy 0.002645 0.246907)
					(xy -0.095739 0.148522)
				)
				(width 0.191479)
			)
		)
	)
	(pad "" smd custom
		(at 1.0875 1.0875)
		(size 0.248041 0.248041)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.095739 0.038978)
					(xy 0.038978 -0.095739)
					(xy 0.095739 -0.095739)
					(xy 0.095739 0.095739)
					(xy -0.095739 0.095739)
				)
				(width 0.191479)
			)
		)
	)
	(pad "1" smd custom
		(at -1.95 -1.4)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.35 -0.05)
					(xy 0.279289 -0.05)
					(xy 0.35 0.020711)
					(xy 0.35 0.05)
					(xy -0.35 0.05)
				)
				(width 0.1)
			)
		)
	)
	(pad "2" smd roundrect
		(at -1.95 -1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.95 -0.6)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.95 -0.2)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.95 0.2)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.95 0.6)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.95 1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd custom
		(at -1.95 1.4)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.35 -0.05)
					(xy 0.35 -0.05)
					(xy 0.35 -0.020711)
					(xy 0.279289 0.05)
					(xy -0.35 0.05)
				)
				(width 0.1)
			)
		)
	)
	(pad "9" smd custom
		(at -1.4 1.95)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.279289)
					(xy 0.020711 -0.35)
					(xy 0.05 -0.35)
					(xy 0.05 0.35)
					(xy -0.05 0.35)
				)
				(width 0.1)
			)
		)
	)
	(pad "10" smd roundrect
		(at -1 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -0.6 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -0.2 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.2 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.6 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd custom
		(at 1.4 1.95)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.35)
					(xy -0.020711 -0.35)
					(xy 0.05 -0.279289)
					(xy 0.05 0.35)
					(xy -0.05 0.35)
				)
				(width 0.1)
			)
		)
	)
	(pad "17" smd custom
		(at 1.95 1.4)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.35 -0.05)
					(xy 0.35 -0.05)
					(xy 0.35 0.05)
					(xy -0.279289 0.05)
					(xy -0.35 -0.020711)
				)
				(width 0.1)
			)
		)
	)
	(pad "18" smd roundrect
		(at 1.95 1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.95 0.6)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.95 0.2)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 1.95 -0.2)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.95 -0.6)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1.95 -1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd custom
		(at 1.95 -1.4)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.35 0.020711)
					(xy -0.279289 -0.05)
					(xy 0.35 -0.05)
					(xy 0.35 0.05)
					(xy -0.35 0.05)
				)
				(width 0.1)
			)
		)
	)
	(pad "25" smd custom
		(at 1.4 -1.95)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.35)
					(xy 0.05 -0.35)
					(xy 0.05 0.279289)
					(xy -0.020711 0.35)
					(xy -0.05 0.35)
				)
				(width 0.1)
			)
		)
	)
	(pad "26" smd roundrect
		(at 1 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 0.6 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 0.2 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -0.2 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -0.6 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -1 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd custom
		(at -1.4 -1.95)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.35)
					(xy 0.05 -0.35)
					(xy 0.05 0.35)
					(xy 0.020711 0.35)
					(xy -0.05 0.279289)
				)
				(width 0.1)
			)
		)
	)
	(pad "33" thru_hole circle
		(at -0.85 -0.85)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.85 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.85 0.85)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0 -0.85)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 2.2 2.2)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 2.65 2.65)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "33" thru_hole circle
		(at 0 0.85)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.85 -0.85)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.85 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.85 0.85)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-32-1EP_4x4mm_P0.4mm_EP2.65x2.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
