(footprint "QFN-32-1EP_7x7mm_P0.65mm_EP4.65x4.65mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 32 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8209-8-bit%20AVR%20ATmega16M1-32M1-64M1_Datasheet.pdf#page=426), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -4.81 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-32-1EP_7x7mm_P0.65mm_EP4.65x4.65mm_ThermalVias"
		(at 0 4.81 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.95 -1.95)
		(size 0.507434 0.507434)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.205099 -0.205099)
					(xy 0.205099 -0.205099)
					(xy 0.205099 0.124546)
					(xy 0.124546 0.205099)
					(xy -0.205099 0.205099)
				)
				(width 0.194471)
			)
		)
	)
	(pad "" smd custom
		(at -1.95 -1.05)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.225652 -0.346586)
					(xy 0.162126 -0.346586)
					(xy 0.225652 -0.28306)
					(xy 0.225652 0.28306)
					(xy 0.162126 0.346586)
					(xy -0.225652 0.346586)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at -1.95 0)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.225652 -0.346586)
					(xy 0.162126 -0.346586)
					(xy 0.225652 -0.28306)
					(xy 0.225652 0.28306)
					(xy 0.162126 0.346586)
					(xy -0.225652 0.346586)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at -1.95 1.05)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.225652 -0.346586)
					(xy 0.162126 -0.346586)
					(xy 0.225652 -0.28306)
					(xy 0.225652 0.28306)
					(xy 0.162126 0.346586)
					(xy -0.225652 0.346586)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at -1.95 1.95)
		(size 0.507434 0.507434)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.205099 -0.205099)
					(xy 0.124546 -0.205099)
					(xy 0.205099 -0.124546)
					(xy 0.205099 0.205099)
					(xy -0.205099 0.205099)
				)
				(width 0.194471)
			)
		)
	)
	(pad "" smd custom
		(at -1.05 -1.95)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.346586 -0.225652)
					(xy 0.346586 -0.225652)
					(xy 0.346586 0.162126)
					(xy 0.28306 0.225652)
					(xy -0.28306 0.225652)
					(xy -0.346586 0.162126)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd roundrect
		(at -1.05 -1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.05 0)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.05 1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at -1.05 1.95)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.346586 -0.162126)
					(xy -0.28306 -0.225652)
					(xy 0.28306 -0.225652)
					(xy 0.346586 -0.162126)
					(xy 0.346586 0.225652)
					(xy -0.346586 0.225652)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 0 -1.95)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.346586 -0.225652)
					(xy 0.346586 -0.225652)
					(xy 0.346586 0.162126)
					(xy 0.28306 0.225652)
					(xy -0.28306 0.225652)
					(xy -0.346586 0.162126)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd roundrect
		(at 0 -1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at 0 1.95)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.346586 -0.162126)
					(xy -0.28306 -0.225652)
					(xy 0.28306 -0.225652)
					(xy 0.346586 -0.162126)
					(xy 0.346586 0.225652)
					(xy -0.346586 0.225652)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 1.05 -1.95)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.346586 -0.225652)
					(xy 0.346586 -0.225652)
					(xy 0.346586 0.162126)
					(xy 0.28306 0.225652)
					(xy -0.28306 0.225652)
					(xy -0.346586 0.162126)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd roundrect
		(at 1.05 -1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.05 0)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.05 1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at 1.05 1.95)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.346586 -0.162126)
					(xy -0.28306 -0.225652)
					(xy 0.28306 -0.225652)
					(xy 0.346586 -0.162126)
					(xy 0.346586 0.225652)
					(xy -0.346586 0.225652)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 1.95 -1.95)
		(size 0.507434 0.507434)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.205099 -0.205099)
					(xy 0.205099 -0.205099)
					(xy 0.205099 0.205099)
					(xy -0.124546 0.205099)
					(xy -0.205099 0.124546)
				)
				(width 0.194471)
			)
		)
	)
	(pad "" smd custom
		(at 1.95 -1.05)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.225652 -0.28306)
					(xy -0.162126 -0.346586)
					(xy 0.225652 -0.346586)
					(xy 0.225652 0.346586)
					(xy -0.162126 0.346586)
					(xy -0.225652 0.28306)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 1.95 0)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.225652 -0.28306)
					(xy -0.162126 -0.346586)
					(xy 0.225652 -0.346586)
					(xy 0.225652 0.346586)
					(xy -0.162126 0.346586)
					(xy -0.225652 0.28306)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 1.95 1.05)
		(size 0.527986 0.527986)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.225652 -0.28306)
					(xy -0.162126 -0.346586)
					(xy 0.225652 -0.346586)
					(xy 0.225652 0.346586)
					(xy -0.162126 0.346586)
					(xy -0.225652 0.28306)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 1.95 1.95)
		(size 0.507434 0.507434)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.205099 -0.124546)
					(xy -0.124546 -0.205099)
					(xy 0.205099 -0.205099)
					(xy 0.205099 0.205099)
					(xy -0.205099 0.205099)
				)
				(width 0.194471)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.3375 -2.275)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.3375 -1.625)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.3375 -0.975)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.3375 -0.325)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.3375 0.325)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.3375 0.975)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.3375 1.625)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.3375 2.275)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -2.275 3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -1.625 3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -0.975 3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -0.325 3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.325 3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.975 3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.625 3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.275 3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 3.3375 2.275)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 3.3375 1.625)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 3.3375 0.975)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 3.3375 0.325)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 3.3375 -0.325)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 3.3375 -0.975)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 3.3375 -1.625)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 3.3375 -2.275)
		(size 1.025 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 2.275 -3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 1.625 -3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 0.975 -3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 0.325 -3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -0.325 -3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -0.975 -3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -1.625 -3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -2.275 -3.3375)
		(size 0.35 1.025)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" thru_hole circle
		(at -1.575 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -1.575 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -1.575 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -1.575 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.525 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.525 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.525 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.525 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 3.65 3.65)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 4.65 4.65)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "33" thru_hole circle
		(at 0.525 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.525 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.525 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.525 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.575 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.575 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.575 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.575 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-32-1EP_7x7mm_P0.65mm_EP4.65x4.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
