(footprint "QFN-32-1EP_7x7mm_P0.65mm_EP5.4x5.4mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 32 Pin (http://www.thatcorp.com/datashts/THAT_5171_Datasheet.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -4.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-32-1EP_7x7mm_P0.65mm_EP5.4x5.4mm"
		(at 0 4.83 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.025 -2.025)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at -2.025 -0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at -2.025 0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at -2.025 2.025)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at -0.675 -2.025)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at -0.675 -0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at -0.675 0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at -0.675 2.025)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at 0.675 -2.025)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at 0.675 -0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at 0.675 0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at 0.675 2.025)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at 2.025 -2.025)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at 2.025 -0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at 2.025 0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "" smd roundrect
		(at 2.025 2.025)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
	)
	(pad "1" smd roundrect
		(at -3.45 -2.275)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.45 -1.625)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.45 -0.975)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.45 -0.325)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.45 0.325)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.45 0.975)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.45 1.625)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.45 2.275)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -2.275 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -1.625 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -0.975 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -0.325 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.325 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.975 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.625 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.275 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 3.45 2.275)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 3.45 1.625)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 3.45 0.975)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 3.45 0.325)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 3.45 -0.325)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 3.45 -0.975)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 3.45 -1.625)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 3.45 -2.275)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 2.275 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 1.625 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 0.975 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 0.325 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -0.325 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -0.975 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -1.625 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -2.275 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 5.4 5.4)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-32-1EP_7x7mm_P0.65mm_EP5.4x5.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
