(footprint "QFN-32-1EP_7x7mm_P0.65mm_EP5.4x5.4mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 32 Pin (http://www.thatcorp.com/datashts/THAT_5171_Datasheet.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -4.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-32-1EP_7x7mm_P0.65mm_EP5.4x5.4mm_ThermalVias"
		(at 0 4.83 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -2.4 -2.4)
		(size 0.365947 0.365947)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.124079 -0.124079)
					(xy 0.124079 -0.124079)
					(xy 0.124079 0.0265)
					(xy 0.0265 0.124079)
					(xy -0.124079 0.124079)
				)
				(width 0.235577)
			)
		)
	)
	(pad "" smd custom
		(at -2.4 -1.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178887 -0.501377)
					(xy 0.126712 -0.501377)
					(xy 0.178887 -0.449202)
					(xy 0.178887 0.449202)
					(xy 0.126712 0.501377)
					(xy -0.178887 0.501377)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at -2.4 0)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178887 -0.501377)
					(xy 0.126712 -0.501377)
					(xy 0.178887 -0.449202)
					(xy 0.178887 0.449202)
					(xy 0.126712 0.501377)
					(xy -0.178887 0.501377)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at -2.4 1.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178887 -0.501377)
					(xy 0.126712 -0.501377)
					(xy 0.178887 -0.449202)
					(xy 0.178887 0.449202)
					(xy 0.126712 0.501377)
					(xy -0.178887 0.501377)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at -2.4 2.4)
		(size 0.365947 0.365947)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.124079 -0.124079)
					(xy 0.0265 -0.124079)
					(xy 0.124079 -0.0265)
					(xy 0.124079 0.124079)
					(xy -0.124079 0.124079)
				)
				(width 0.235577)
			)
		)
	)
	(pad "" smd custom
		(at -1.4 -2.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.501377 -0.178887)
					(xy 0.501377 -0.178887)
					(xy 0.501377 0.126712)
					(xy 0.449202 0.178887)
					(xy -0.449202 0.178887)
					(xy -0.501377 0.126712)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd roundrect
		(at -1.4 -1.4)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd roundrect
		(at -1.4 0)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd roundrect
		(at -1.4 1.4)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd custom
		(at -1.4 2.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.501377 -0.126712)
					(xy -0.449202 -0.178887)
					(xy 0.449202 -0.178887)
					(xy 0.501377 -0.126712)
					(xy 0.501377 0.178887)
					(xy -0.501377 0.178887)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at 0 -2.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.501377 -0.178887)
					(xy 0.501377 -0.178887)
					(xy 0.501377 0.126712)
					(xy 0.449202 0.178887)
					(xy -0.449202 0.178887)
					(xy -0.501377 0.126712)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd roundrect
		(at 0 -1.4)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd roundrect
		(at 0 1.4)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd custom
		(at 0 2.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.501377 -0.126712)
					(xy -0.449202 -0.178887)
					(xy 0.449202 -0.178887)
					(xy 0.501377 -0.126712)
					(xy 0.501377 0.178887)
					(xy -0.501377 0.178887)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at 1.4 -2.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.501377 -0.178887)
					(xy 0.501377 -0.178887)
					(xy 0.501377 0.126712)
					(xy 0.449202 0.178887)
					(xy -0.449202 0.178887)
					(xy -0.501377 0.126712)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd roundrect
		(at 1.4 -1.4)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd roundrect
		(at 1.4 0)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd roundrect
		(at 1.4 1.4)
		(size 1.128716 1.128716)
		(layers "F.Paste")
		(roundrect_rratio 0.221491)
	)
	(pad "" smd custom
		(at 1.4 2.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.501377 -0.126712)
					(xy -0.449202 -0.178887)
					(xy 0.449202 -0.178887)
					(xy 0.501377 -0.126712)
					(xy 0.501377 0.178887)
					(xy -0.501377 0.178887)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at 2.4 -2.4)
		(size 0.365947 0.365947)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.124079 -0.124079)
					(xy 0.124079 -0.124079)
					(xy 0.124079 0.124079)
					(xy -0.0265 0.124079)
					(xy -0.124079 0.0265)
				)
				(width 0.235577)
			)
		)
	)
	(pad "" smd custom
		(at 2.4 -1.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178887 -0.449202)
					(xy -0.126712 -0.501377)
					(xy 0.178887 -0.501377)
					(xy 0.178887 0.501377)
					(xy -0.126712 0.501377)
					(xy -0.178887 0.449202)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at 2.4 0)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178887 -0.449202)
					(xy -0.126712 -0.501377)
					(xy 0.178887 -0.501377)
					(xy 0.178887 0.501377)
					(xy -0.126712 0.501377)
					(xy -0.178887 0.449202)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at 2.4 1.4)
		(size 0.420755 0.420755)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.178887 -0.449202)
					(xy -0.126712 -0.501377)
					(xy 0.178887 -0.501377)
					(xy 0.178887 0.501377)
					(xy -0.126712 0.501377)
					(xy -0.178887 0.449202)
				)
				(width 0.125962)
			)
		)
	)
	(pad "" smd custom
		(at 2.4 2.4)
		(size 0.365947 0.365947)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.124079 -0.0265)
					(xy -0.0265 -0.124079)
					(xy 0.124079 -0.124079)
					(xy 0.124079 0.124079)
					(xy -0.124079 0.124079)
				)
				(width 0.235577)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.45 -2.275)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.45 -1.625)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.45 -0.975)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.45 -0.325)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.45 0.325)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.45 0.975)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.45 1.625)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.45 2.275)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -2.275 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -1.625 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -0.975 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -0.325 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.325 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.975 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.625 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.275 3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 3.45 2.275)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 3.45 1.625)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 3.45 0.975)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 3.45 0.325)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 3.45 -0.325)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 3.45 -0.975)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 3.45 -1.625)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 3.45 -2.275)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 2.275 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 1.625 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 0.975 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 0.325 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -0.325 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -0.975 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -1.625 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -2.275 -3.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" thru_hole circle
		(at -2.1 -2.1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -2.1 -0.7)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -2.1 0.7)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -2.1 2.1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.7 -2.1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.7 -0.7)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.7 0.7)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.7 2.1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 4.7 4.7)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 5.4 5.4)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "33" thru_hole circle
		(at 0.7 -2.1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.7 -0.7)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.7 0.7)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.7 2.1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 2.1 -2.1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 2.1 -0.7)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 2.1 0.7)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 2.1 2.1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-32-1EP_7x7mm_P0.65mm_EP5.4x5.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
