(footprint "QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 40 Pin (http://www.issi.com/WW/pdf/31FL3736.pdf#page=28), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm_ThermalVias"
		(at 0 3.83 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.1 -1.1)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "" smd custom
		(at -1.1 0)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "" smd custom
		(at -1.1 1.1)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "" smd custom
		(at 0 -1.1)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "" smd custom
		(at 0 0)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "" smd custom
		(at 0 1.1)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "" smd custom
		(at 1.1 -1.1)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "" smd custom
		(at 1.1 0)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "" smd custom
		(at 1.1 1.1)
		(size 0.865191 0.865191)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.374613 -0.278545)
					(xy -0.278545 -0.374613)
					(xy 0.278545 -0.374613)
					(xy 0.374613 -0.278545)
					(xy 0.374613 0.278545)
					(xy 0.278545 0.374613)
					(xy -0.278545 0.374613)
					(xy -0.374613 0.278545)
				)
				(width 0.231929)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.4875 -1.8)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.4875 -1.4)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.4875 -1)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.4875 -0.6)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.4875 -0.2)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.4875 0.2)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.4875 0.6)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -2.4875 1)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -2.4875 1.4)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -2.4875 1.8)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -1.8 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -1.4 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -1 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -0.6 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -0.2 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 0.2 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 0.6 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.4 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.8 2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.4875 1.8)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 2.4875 1.4)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 2.4875 1)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.4875 0.6)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 2.4875 0.2)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 2.4875 -0.2)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 2.4875 -0.6)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 2.4875 -1)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 2.4875 -1.4)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 2.4875 -1.8)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 1.8 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 1.4 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 1 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 0.6 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 0.2 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -0.2 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at -0.6 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at -1 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at -1.4 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at -1.8 -2.4875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" thru_hole circle
		(at -1.65 -1.65)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -1.65 -0.55)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -1.65 0.55)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -1.65 1.65)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -0.55 -1.65)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -0.55 -0.55)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -0.55 0.55)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -0.55 1.65)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" smd rect
		(at 0 0)
		(size 3.8 3.8)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at 0 0)
		(size 3.8 3.8)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "41" thru_hole circle
		(at 0.55 -1.65)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.55 -0.55)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.55 0.55)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.55 1.65)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.65 -1.65)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.65 -0.55)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.65 0.55)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.65 1.65)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
