(footprint "QFN-44-1EP_9x9mm_P0.65mm_EP7.5x7.5mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "44-Lead Plastic Quad Flat, No Lead Package - 9x9 mm Body [QFN] with thermal vias; see section 10.3 of https://www.parallax.com/sites/default/files/downloads/P8X32A-Propeller-Datasheet-v1.4.0_0.pdf")
	(tags "QFN 0.65")
	(property "Reference" "REF**"
		(at 0 -5.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-44-1EP_9x9mm_P0.65mm_EP7.5x7.5mm_ThermalVias"
		(at 0 5.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.875 -1.875)
		(size 2.65 2.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.875 1.875)
		(size 2.65 2.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.875 -1.875)
		(size 2.65 2.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.875 1.875)
		(size 2.65 2.65)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -4.3 -3.25)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.3 -2.6)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.3 -1.95)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.3 -1.3)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.3 -0.65)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.3 0)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.3 0.65)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.3 1.3)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -4.3 1.95)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -4.3 2.6)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -4.3 3.25)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.25 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -2.6 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -1.95 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.3 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -0.65 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 0 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 0.65 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.3 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.95 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 2.6 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 3.25 4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 4.3 3.25)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 4.3 2.6)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 4.3 1.95)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 4.3 1.3)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 4.3 0.65)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 4.3 0)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 4.3 -0.65)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 4.3 -1.3)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 4.3 -1.95)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 4.3 -2.6)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 4.3 -3.25)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.25 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 2.6 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 1.95 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 1.3 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 0.65 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 0 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -0.65 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -1.3 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at -1.95 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -2.6 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -3.25 -4.3 90)
		(size 0.6 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" thru_hole circle
		(at -1.875 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "45" thru_hole circle
		(at 0 -1.875)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "45" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "45" smd rect
		(at 0 0)
		(size 7.5 7.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "45" smd rect
		(at 0 0)
		(size 8.5 8.5)
		(layers "B.Cu")
	)
	(pad "45" thru_hole circle
		(at 0 1.875)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "45" thru_hole circle
		(at 1.875 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-44-1EP_9x9mm_Pitch0.65mm_EP7.5x7.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
