(footprint "QFN-56-1EP_8x8mm_P0.5mm_EP4.5x5.2mm_ThermalVias_TopTented"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "QFN, 56 Pin top tented version (manually modified). For information see: http://www.cypress.com/file/138911/download")
	(tags "QFN DFN_QFN")
	(property "Reference" "REF**"
		(at 0 -5.32 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-56-1EP_8x8mm_P0.5mm_EP4.5x5.2mm_ThermalVias_TopTented"
		(at 0 5.32 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.5 -1.7625)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.837549) (xy 0.3 -0.837549)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.75 0.3675) (xy -0.75 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -1.5 -1.7625)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -1.5 -0.5875)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.75 0.3675) (xy -0.75 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -1.5 -0.5875)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -1.5 0.5875)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.75 0.3675) (xy -0.75 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -1.5 0.5875)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -1.5 1.7625)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 0.837549) (xy -0.3 0.837549) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.75 0.3675) (xy -0.75 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -1.5 1.7625)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 -1.7625)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.837549) (xy 0.3 -0.837549)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 -1.7625)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 -0.5875)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 -0.5875)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 0.5875)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 0.5875)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 1.7625)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.837549) (xy -0.3 0.837549) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 1.7625)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 -1.7625)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.837549) (xy 0.3 -0.837549)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 -1.7625)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 -0.5875)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 -0.5875)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 0.5875)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 0.5875)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 1.7625)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.837549) (xy -0.3 0.837549) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.5 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 1.7625)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.5 -1.7625)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.75 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.75 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.837549) (xy 0.3 -0.837549)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.5 -1.7625)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.5 -0.5875)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.75 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.75 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.5 -0.5875)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.5 0.5875)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.75 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.75 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.5875) (xy -0.3 0.5875) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.5 0.5875)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.5 1.7625)
		(size 0.776286 0.776286)
		(layers "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -0.5025) (xy -0.3 -0.5025) (xy -0.3 -0.5875) (xy 0.3 -0.5875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.75 0.3675) (xy 0.435 0.3675) (xy 0.435 -0.3675) (xy 0.75 -0.3675)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.435 -0.3675) (xy 0.435 0.3675) (xy 0.3 0.5025) (xy -0.3 0.5025) (xy -0.435 0.3675) (xy -0.435 -0.3675)
					(xy -0.3 -0.5025) (xy 0.3 -0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.3 0.837549) (xy -0.3 0.837549) (xy -0.3 0.5025) (xy 0.3 0.5025)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.435 0.3675) (xy -0.5 0.3675) (xy -0.5 -0.3675) (xy -0.435 -0.3675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.5 1.7625)
		(size 0.776286 0.776286)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.435 -0.3575) (xy 0.435 0.3575) (xy 0.29 0.5025) (xy -0.29 0.5025) (xy -0.435 0.3575) (xy -0.435 -0.3575)
					(xy -0.29 -0.5025) (xy 0.29 -0.5025)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.9375 -3.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.9375 -2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.9375 -2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.9375 -1.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.9375 -1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.9375 -0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.9375 -0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.9375 0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -3.9375 0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -3.9375 1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -3.9375 1.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -3.9375 2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -3.9375 2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -3.9375 3.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -3.25 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -2.75 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -2.25 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -1.75 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -1.25 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -0.75 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -0.25 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 0.25 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 0.75 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 1.25 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 1.75 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 2.25 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 2.75 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 3.25 3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 3.9375 3.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 3.9375 2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 3.9375 2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 3.9375 1.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 3.9375 1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 3.9375 0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 3.9375 0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 3.9375 -0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 3.9375 -0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 3.9375 -1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 3.9375 -1.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 3.9375 -2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 3.9375 -2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 3.9375 -3.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 3.25 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at 2.75 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 2.25 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 1.75 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at 1.25 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at 0.75 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at 0.25 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at -0.25 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at -0.75 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at -1.25 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at -1.75 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at -2.25 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at -2.75 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at -3.25 -3.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "57" thru_hole circle
		(at -2 -2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -2 -1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -2 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -2 1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -2 2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -1 -2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -1 -1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -1 1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at -1 2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 0 -2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 0 -1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" smd roundrect
		(at 0 0)
		(size 4.5 5.2)
		(layers "F.Cu")
		(roundrect_rratio 0.056)
	)
	(pad "57" smd roundrect
		(at 0 0)
		(size 4.5 5.2)
		(layers "B.Cu")
		(roundrect_rratio 0.055556)
	)
	(pad "57" thru_hole circle
		(at 0 1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 0 2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 1 -2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 1 -1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 1 1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 1 2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 2 -2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 2 -1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 2 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 2 1.175)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 2 2.35)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_8x8mm_P0.5mm_EP4.5x5.2mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
