(footprint "QFN-64-1EP_9x9mm_P0.5mm_EP7.25x7.25mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "64-Lead Plastic Quad Flat No-Lead Package, 9x9mm Body (see Atmel Appnote 8826)")
	(tags "QFN 0.5")
	(property "Reference" "REF**"
		(at 0 -5.875 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-64-1EP_9x9mm_P0.5mm_EP7.25x7.25mm"
		(at 0 5.875 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -2.8 -2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.8 -1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.8 0)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.8 1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.8 2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 -2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 -1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 0)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 -2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 -1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 0)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.8 -2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.8 -1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.8 0)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.8 1.4)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.8 2.8)
		(size 1.19 1.19)
		(layers "F.Paste")
	)
	(pad "1" smd oval
		(at -4.5 -3.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -4.5 -3.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -4.5 -2.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -4.5 -2.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -4.5 -1.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -4.5 -1.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -4.5 -0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -4.5 -0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -4.5 0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -4.5 0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -4.5 1.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -4.5 1.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at -4.5 2.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at -4.5 2.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -4.5 3.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -4.5 3.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at -3.75 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at -3.25 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at -2.75 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at -2.25 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at -1.75 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at -1.25 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at -0.75 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at -0.25 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at 0.25 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 0.75 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 1.25 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 1.75 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at 2.25 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 2.75 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 3.25 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 3.75 4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 4.5 3.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at 4.5 3.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at 4.5 2.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at 4.5 2.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at 4.5 1.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at 4.5 1.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd oval
		(at 4.5 0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd oval
		(at 4.5 0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd oval
		(at 4.5 -0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd oval
		(at 4.5 -0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd oval
		(at 4.5 -1.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd oval
		(at 4.5 -1.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd oval
		(at 4.5 -2.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd oval
		(at 4.5 -2.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd oval
		(at 4.5 -3.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd oval
		(at 4.5 -3.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd oval
		(at 3.75 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd oval
		(at 3.25 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd oval
		(at 2.75 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd oval
		(at 2.25 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd oval
		(at 1.75 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd oval
		(at 1.25 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd oval
		(at 0.75 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd oval
		(at 0.25 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd oval
		(at -0.25 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd oval
		(at -0.75 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd oval
		(at -1.25 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd oval
		(at -1.75 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd oval
		(at -2.25 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd oval
		(at -2.75 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd oval
		(at -3.25 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd oval
		(at -3.75 -4.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at 0 0)
		(size 7.25 7.25)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-64-1EP_9x9mm_P0.5mm_EP7.25x7.25mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
