(footprint "QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 68 Pin (https://www.st.com/resource/en/datasheet/stm32h725ze.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -5.31 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm_ThermalVias"
		(at 0 5.31 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.2125 -2.2125)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at -2.2125 -0.7375)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at -2.2125 0.7375)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at -2.2125 2.2125)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at -0.7375 -2.2125)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at -0.7375 -0.7375)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at -0.7375 0.7375)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at -0.7375 2.2125)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at 0.7375 -2.2125)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at 0.7375 -0.7375)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at 0.7375 0.7375)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at 0.7375 2.2125)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at 2.2125 -2.2125)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at 2.2125 -0.7375)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at 2.2125 0.7375)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "" smd roundrect
		(at 2.2125 2.2125)
		(size 1.239355 1.239355)
		(layers "F.Paste")
		(roundrect_rratio 0.201718)
	)
	(pad "1" smd roundrect
		(at -3.8875 -3.2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.8875 -2.8)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.8875 -2.4)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.8875 -2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.8875 -1.6)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.8875 -1.2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.8875 -0.8)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.8875 -0.4)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -3.8875 0)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -3.8875 0.4)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -3.8875 0.8)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -3.8875 1.2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -3.8875 1.6)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -3.8875 2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -3.8875 2.4)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -3.8875 2.8)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -3.8875 3.2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -3.2 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -2.8 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -2.4 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -2 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -1.6 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -1.2 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -0.8 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at -0.4 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 0 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 0.4 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 0.8 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 1.2 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 1.6 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 2 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 2.4 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 2.8 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 3.2 3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 3.8875 3.2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 3.8875 2.8)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 3.8875 2.4)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 3.8875 2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 3.8875 1.6)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 3.8875 1.2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 3.8875 0.8)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 3.8875 0.4)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 3.8875 0)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at 3.8875 -0.4)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 3.8875 -0.8)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 3.8875 -1.2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at 3.8875 -1.6)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at 3.8875 -2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at 3.8875 -2.4)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at 3.8875 -2.8)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at 3.8875 -3.2)
		(size 0.925 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at 3.2 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at 2.8 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at 2.4 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at 2 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at 1.6 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd roundrect
		(at 1.2 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "58" smd roundrect
		(at 0.8 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "59" smd roundrect
		(at 0.4 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "60" smd roundrect
		(at 0 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "61" smd roundrect
		(at -0.4 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "62" smd roundrect
		(at -0.8 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "63" smd roundrect
		(at -1.2 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "64" smd roundrect
		(at -1.6 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "65" smd roundrect
		(at -2 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "66" smd roundrect
		(at -2.4 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "67" smd roundrect
		(at -2.8 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "68" smd roundrect
		(at -3.2 -3.8875)
		(size 0.25 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "69" thru_hole circle
		(at -2.95 -2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -2.95 -1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -2.95 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -2.95 1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -2.95 2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -1.475 -2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -1.475 -1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -1.475 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -1.475 1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at -1.475 2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 0 -2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 0 -1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" smd rect
		(at 0 0)
		(size 6.4 6.4)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "69" smd rect
		(at 0 0)
		(size 6.4 6.4)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "69" thru_hole circle
		(at 0 1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 0 2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 1.475 -2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 1.475 -1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 1.475 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 1.475 1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 1.475 2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 2.95 -2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 2.95 -1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 2.95 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 2.95 1.475)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 2.95 2.95)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
