(footprint "ST_UFQFPN-20_3x3mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "UFQFPN 20-lead, 3 x 3 mm, 0.5 mm pitch, ultra thin fine pitch quad flat package (http://www.st.com/resource/en/datasheet/stm8s003f3.pdf)")
	(tags "UFQFPN 0.5")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_UFQFPN-20_3x3mm_P0.5mm"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -1.475 -1)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.325 0) (xy 0.325 0.15) (xy 0.175 0.15) (xy 0.175 -0.15)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd rect
		(at -1.3 -0.5)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.3 0)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.3 0.5)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd custom
		(at -1.475 1)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.325 0) (xy 0.175 0.15) (xy 0.175 -0.15) (xy 0.325 -0.15)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "6" smd custom
		(at -1 1.475)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.15 -0.175) (xy -0.15 -0.175) (xy 0 -0.325) (xy 0.15 -0.325)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "7" smd rect
		(at -0.5 1.3)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0 1.3)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.5 1.3)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd custom
		(at 1 1.475)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.15 -0.175) (xy -0.15 -0.175) (xy -0.15 -0.325) (xy 0 -0.325)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "11" smd custom
		(at 1.475 1)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.175 0.15) (xy -0.325 0) (xy -0.325 -0.15) (xy -0.175 -0.15)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "12" smd rect
		(at 1.3 0.5)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.3 0)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.3 -0.5)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd custom
		(at 1.475 -1)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.175 0.15) (xy -0.325 0.15) (xy -0.325 0) (xy -0.175 -0.15)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "16" smd custom
		(at 1 -1.475)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0.325) (xy -0.15 0.325) (xy -0.15 0.175) (xy 0.15 0.175)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "17" smd rect
		(at 0.5 -1.3)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 0 -1.3)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -0.5 -1.3)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd custom
		(at -1 -1.475)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.15 0.325) (xy 0 0.325) (xy -0.15 0.175) (xy 0.15 0.175)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/ST_UFQFPN-20_3x3mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
