(footprint "ST_UQFN-6L_1.5x1.7mm_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ST  UQFN, 6 Pin (https://www.st.com/resource/en/datasheet/ecmf02-2amx6.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "ST UQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_UQFN-6L_1.5x1.7mm_P0.5mm"
		(at 0 1.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.6875 -0.5)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.6875 0)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.6875 0.5)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.6875 0.5)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.6875 0)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.6875 -0.5)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/ST_UQFN-6L_1.5x1.7mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
