(footprint "TDFN-8-1EP_3x2mm_P0.5mm_EP1.4x1.4mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TDFN, 8 Pin (http://ww1.microchip.com/downloads/en/devicedoc/20005514a.pdf#page=35), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "TDFN NoLead")
	(property "Reference" "REF**"
		(at 0 -1.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "TDFN-8-1EP_3x2mm_P0.5mm_EP1.4x1.4mm"
		(at 0 1.95 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.35 -0.35)
		(size 0.56 0.56)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.35 0.35)
		(size 0.56 0.56)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.35 -0.35)
		(size 0.56 0.56)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.35 0.35)
		(size 0.56 0.56)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.4625 -0.75)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.4625 -0.25)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.4625 0.25)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.4625 0.75)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 1.4625 0.75)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 1.4625 0.25)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1.4625 -0.25)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.4625 -0.75)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.4 1.4)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TDFN-8-1EP_3x2mm_P0.5mm_EP1.4x1.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
