(footprint "TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-lead plastic dual flat, 2x3x0.75mm size, 0.5mm pitch (http://ww1.microchip.com/downloads/en/DeviceDoc/8L_TDFN_2x3_MN_C04-0129E-MN.pdf)")
	(tags "TDFN DFN 0.5mm")
	(property "Reference" "REF**"
		(at 0 -1.88 0)
		(layer "F.SilkS")
	)
	(property "Value" "TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm_ThermalVias"
		(at 0 1.88 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at 0 -0.5)
		(size 0.7 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 1.8 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0.5)
		(size 0.7 0.65)
		(layers "F.Paste")
	)
	(pad "1" smd oval
		(at -1.45 -0.75)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -1.45 -0.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -1.45 0.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -1.45 0.75)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at 1.45 0.75)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at 1.45 0.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at 1.45 -0.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 1.45 -0.75)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" thru_hole circle
		(at -0.5 -0.5)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -0.5 0.5)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.8 1.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.8 1.65)
		(layers "B.Cu")
	)
	(pad "9" thru_hole circle
		(at 0.5 -0.5)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0.5 0.5)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
