(footprint "TQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TQFN, 32 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0140.PDF (T3255-3)), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "TQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "TQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
		(at 0 3.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.775 -0.775)
		(size 1.25 1.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at -0.775 0.775)
		(size 1.25 1.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.775 -0.775)
		(size 1.25 1.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.775 0.775)
		(size 1.25 1.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "1" smd custom
		(at -2.4375 -1.75)
		(size 0.18636 0.18636)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.35 -0.0625)
					(xy 0.296612 -0.0625)
					(xy 0.35 -0.009112)
					(xy 0.35 0.0625)
					(xy -0.35 0.0625)
				)
				(width 0.125)
			)
		)
	)
	(pad "2" smd roundrect
		(at -2.4375 -1.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.4375 -0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.4375 -0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.4375 0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.4375 0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.4375 1.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd custom
		(at -2.4375 1.75)
		(size 0.18636 0.18636)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.35 -0.0625)
					(xy 0.35 -0.0625)
					(xy 0.35 0.009112)
					(xy 0.296612 0.0625)
					(xy -0.35 0.0625)
				)
				(width 0.125)
			)
		)
	)
	(pad "9" smd custom
		(at -1.75 2.4375)
		(size 0.18636 0.18636)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.0625 -0.296612)
					(xy -0.009112 -0.35)
					(xy 0.0625 -0.35)
					(xy 0.0625 0.35)
					(xy -0.0625 0.35)
				)
				(width 0.125)
			)
		)
	)
	(pad "10" smd roundrect
		(at -1.25 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -0.75 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -0.25 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.25 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.75 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.25 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd custom
		(at 1.75 2.4375)
		(size 0.18636 0.18636)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.0625 -0.35)
					(xy 0.009112 -0.35)
					(xy 0.0625 -0.296612)
					(xy 0.0625 0.35)
					(xy -0.0625 0.35)
				)
				(width 0.125)
			)
		)
	)
	(pad "17" smd custom
		(at 2.4375 1.75)
		(size 0.18636 0.18636)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.35 -0.0625)
					(xy 0.35 -0.0625)
					(xy 0.35 0.0625)
					(xy -0.296612 0.0625)
					(xy -0.35 0.009112)
				)
				(width 0.125)
			)
		)
	)
	(pad "18" smd roundrect
		(at 2.4375 1.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 2.4375 0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.4375 0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.4375 -0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 2.4375 -0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 2.4375 -1.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd custom
		(at 2.4375 -1.75)
		(size 0.18636 0.18636)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.35 -0.009112)
					(xy -0.296612 -0.0625)
					(xy 0.35 -0.0625)
					(xy 0.35 0.0625)
					(xy -0.35 0.0625)
				)
				(width 0.125)
			)
		)
	)
	(pad "25" smd custom
		(at 1.75 -2.4375)
		(size 0.18636 0.18636)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.0625 -0.35)
					(xy 0.0625 -0.35)
					(xy 0.0625 0.296612)
					(xy 0.009112 0.35)
					(xy -0.0625 0.35)
				)
				(width 0.125)
			)
		)
	)
	(pad "26" smd roundrect
		(at 1.25 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 0.75 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 0.25 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -0.25 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -0.75 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -1.25 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd custom
		(at -1.75 -2.4375)
		(size 0.18636 0.18636)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.0625 -0.35)
					(xy 0.0625 -0.35)
					(xy 0.0625 0.35)
					(xy -0.009112 0.35)
					(xy -0.0625 0.296612)
				)
				(width 0.125)
			)
		)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 3.1 3.1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
