(footprint "Texas_B3QFN-14-1EP_5x5.5mm_P0.65mm_ThermalVia"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas instruments QFN Package, datasheet: https://www.ti.com/lit/ds/symlink/tpsm53602.pdf")
	(tags "Texas instruments QFN")
	(property "Reference" "REF**"
		(at 0 -3.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_B3QFN-14-1EP_5x5.5mm_P0.65mm_ThermalVia"
		(at 0 3.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.625 -0.475)
		(size 0.95 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.077)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at -0.625 0.475)
		(size 0.95 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.077)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at -0.425 -1.675)
		(size 0.6 1.15)
		(layers "F.Paste")
		(roundrect_rratio 0.083)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at -0.425 1.675)
		(size 0.6 1.15)
		(layers "F.Paste")
		(roundrect_rratio 0.083)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0.425 -1.675)
		(size 0.6 1.15)
		(layers "F.Paste")
		(roundrect_rratio 0.083)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0.425 1.675)
		(size 0.6 1.15)
		(layers "F.Paste")
		(roundrect_rratio 0.083)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0.625 -0.475)
		(size 0.95 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.077)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0.625 0.475)
		(size 0.95 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.077)
		(zone_connect 0)
	)
	(pad "1" smd roundrect
		(at -2 -2.145)
		(size 1.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at -2.35 -1.17)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "3" smd roundrect
		(at -2.35 -0.52)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "4" smd roundrect
		(at -2.35 0.13)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "5" smd roundrect
		(at -2.35 0.78)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "6" smd roundrect
		(at -2.35 1.43)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "7" smd roundrect
		(at -2 2.155)
		(size 1.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "8" smd roundrect
		(at 2 2.155)
		(size 1.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "9" smd roundrect
		(at 2.35 1.43)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "10" smd roundrect
		(at 2.35 0.78)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "11" smd roundrect
		(at 2.35 0.13)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "12" smd roundrect
		(at 2.35 -0.52)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "13" smd roundrect
		(at 2.35 -1.17)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.143)
	)
	(pad "14" smd roundrect
		(at 2 -2.145)
		(size 1.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "15" thru_hole circle
		(at -0.95 -0.95)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at -0.95 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at -0.95 0.95)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at 0 -1.9)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at 0 -0.95)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" smd custom
		(at 0 0)
		(size 2.5 2.5)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.75 -1.25) (xy -0.75 -1.25) (xy -0.75 -2.3) (xy 0.75 -2.3)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.75 2.3) (xy -0.75 2.3) (xy -0.75 1.25) (xy 0.75 1.25)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "15" thru_hole circle
		(at 0 0.95)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at 0 1.9)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at 0.95 -0.95)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at 0.95 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(pad "15" thru_hole circle
		(at 0.95 0.95)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 1)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_B3QFN-14-1EP_5x5.5mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
