(footprint "Texas_DRB0008A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DFN-8, 3x3x1mm, http://www.ti.com/lit/ds/symlink/ucc24610.pdf")
	(tags "DRB0008A")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DRB0008A"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.07)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.325 -1.337)
		(size 0.23 0.725)
		(layers "F.Paste")
		(roundrect_rratio 0.22)
	)
	(pad "" smd roundrect
		(at -0.325 1.337)
		(size 0.23 0.725)
		(layers "F.Paste")
		(roundrect_rratio 0.22)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.34 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.038)
	)
	(pad "" smd roundrect
		(at 0.325 -1.337)
		(size 0.23 0.725)
		(layers "F.Paste")
		(roundrect_rratio 0.22)
	)
	(pad "" smd roundrect
		(at 0.325 1.337)
		(size 0.23 0.725)
		(layers "F.Paste")
		(roundrect_rratio 0.22)
	)
	(pad "1" smd roundrect
		(at -1.4 -0.975)
		(size 0.6 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16)
	)
	(pad "2" smd roundrect
		(at -1.4 -0.325)
		(size 0.6 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16)
	)
	(pad "3" smd roundrect
		(at -1.4 0.325)
		(size 0.6 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16)
	)
	(pad "4" smd roundrect
		(at -1.4 0.975)
		(size 0.6 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16)
	)
	(pad "5" smd roundrect
		(at 1.4 0.975)
		(size 0.6 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16)
	)
	(pad "6" smd roundrect
		(at 1.4 0.325)
		(size 0.6 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16)
	)
	(pad "7" smd roundrect
		(at 1.4 -0.325)
		(size 0.6 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16)
	)
	(pad "8" smd roundrect
		(at 1.4 -0.975)
		(size 0.6 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16)
	)
	(pad "9" thru_hole circle
		(at -0.5 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" smd roundrect
		(at -0.325 -1.1875)
		(size 0.23 1.025)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.22)
	)
	(pad "9" smd roundrect
		(at -0.325 1.1875)
		(size 0.23 1.025)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.22)
	)
	(pad "9" thru_hole circle
		(at 0 -0.625)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" smd roundrect
		(at 0 0)
		(size 1.5 1.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.034)
	)
	(pad "9" smd roundrect
		(at 0 0)
		(size 1.5 1.75)
		(layers "B.Cu")
		(roundrect_rratio 0.034)
	)
	(pad "9" thru_hole circle
		(at 0 0.625)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" smd roundrect
		(at 0.325 -1.1875)
		(size 0.23 1.025)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.22)
	)
	(pad "9" smd roundrect
		(at 0.325 1.1875)
		(size 0.23 1.025)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.22)
	)
	(pad "9" thru_hole circle
		(at 0.5 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_DRB0008A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
