(footprint "Texas_MOF0009A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Instruments, QFM MOF0009A, 6x8x2mm (http://www.ti.com/lit/ml/mpsi063a/mpsi063a.pdf)")
	(tags "ti qfm mof0009a")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_MOF0009A"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin -0.05)
	(solder_paste_margin -0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.55 -3.5575)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at -2.55 -2.6675)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at -2.55 -1.7775)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at -2.55 -0.8875)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at -2.55 0.0025)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 0 -3.5575)
		(size 1.05 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 0 -2.6675)
		(size 1.05 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 0 -1.7775)
		(size 1.05 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 0 -0.8875)
		(size 1.05 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 0 0.0025)
		(size 1.05 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 2.55 -3.5575)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 2.55 -2.6675)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 2.55 -1.7775)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 2.55 -0.8875)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "" smd roundrect
		(at 2.55 0.0025)
		(size 0.7 0.59)
		(layers "F.Paste")
		(roundrect_rratio 0.085)
	)
	(pad "1" smd roundrect
		(at -2.55 -1.7775)
		(size 0.8 4.35)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.063)
	)
	(pad "2" smd roundrect
		(at -2.55 2.0525)
		(size 0.8 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "3" smd roundrect
		(at -2.55 3.2525)
		(size 0.8 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "4" smd roundrect
		(at -0.9 3.5525)
		(size 0.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "5" smd roundrect
		(at 0.9 3.5525)
		(size 0.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "6" smd roundrect
		(at 2.55 3.2525)
		(size 0.8 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "7" smd roundrect
		(at 2.55 2.0525)
		(size 0.8 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "8" smd roundrect
		(at 2.55 -1.7775)
		(size 0.8 4.35)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.063)
	)
	(pad "9" smd roundrect
		(at 0 -1.7775)
		(size 1.15 4.35)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.044)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_MOF0009A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
