(footprint "Texas_PicoStar_DFN-3_0.69x0.60mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Picostar DFN-3, 0.73x0.64mm max, 0.69x0.60mm nom, https://www.ti.com/lit/ds/symlink/csd13380f3.pdf")
	(tags "TI YJM0003A")
	(property "Reference" "REF**"
		(at -0.45 -1.25 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_PicoStar_DFN-3_0.69x0.60mm"
		(at 0 1.35 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 1.35 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 1.35 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.175 -0.2)
		(size 0.25 0.2)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.175 0.2)
		(size 0.25 0.2)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "1" smd roundrect
		(at -0.175 -0.175)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.4)
		(solder_mask_margin -0.05)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -0.175 0.175)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.4)
		(solder_mask_margin -0.05)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at 0.225 0)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.4)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_PicoStar_DFN-3_0.69x0.60mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
