(footprint "Texas_QFN-41_10x16mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "QFN, 41 Pin (http://www.ti.com/lit/ml/mpqf506/mpqf506.pdf)")
	(tags "QFN DFN_QFN")
	(property "Reference" "REF**"
		(at 0 -9.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_QFN-41_10x16mm"
		(at 0 9.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -4.635 -5.6)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.635 -4)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.635 -2.4)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.635 -0.8)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.635 1.2)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.635 5.6)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.285 -7.185)
		(size 0.87 0.87)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.385 0.485) (xy -0.81 0.485) (xy -0.81 0.285) (xy -0.385 0.285) (xy -0.385 -0.375) (xy 0.385 -0.375)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.385 0.085)
				(mid -0.443579 0.226421)
				(end -0.585 0.285)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.285 -7.185)
		(size 0.87 1.07)
		(layers "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.385 0.485) (xy -0.81 0.485) (xy -0.81 0.285) (xy -0.385 0.285) (xy -0.385 -0.485) (xy 0.385 -0.485)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.385 0.085)
				(mid -0.443579 0.226421)
				(end -0.585 0.285)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.285 7.185)
		(size 0.87 0.87)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.385 0.375) (xy -0.385 0.375) (xy -0.385 -0.285) (xy -0.81 -0.285) (xy -0.81 -0.485) (xy 0.385 -0.485)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.585 -0.285)
				(mid -0.443579 -0.226421)
				(end -0.385 -0.085)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -4.285 7.185)
		(size 0.87 1.07)
		(layers "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.385 0.485) (xy -0.385 0.485) (xy -0.385 -0.285) (xy -0.81 -0.285) (xy -0.81 -0.485) (xy 0.385 -0.485)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.585 -0.285)
				(mid -0.443579 -0.226421)
				(end -0.385 -0.085)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -2.4 -7.635 270)
		(size 0.27 1.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.1) (xy -0.465 0.1) (xy -0.465 -0.1) (xy 0.035 -0.1)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.7) (xy -0.465 -0.7) (xy -0.465 -0.9) (xy 0.035 -0.9)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 -0.3)
				(mid -0.093579 -0.158579)
				(end -0.235 -0.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.7)
				(mid -0.093579 -0.641421)
				(end -0.035 -0.5)
				(width 0.2)
			)
			(gr_poly
				(pts
					(xy 0.035 0.9) (xy -0.465 0.9) (xy -0.465 0.7) (xy 0.035 0.7)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.235 0.1)
				(mid -0.093579 0.158579)
				(end -0.035 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.035 0.5)
				(mid -0.093579 0.641421)
				(end -0.235 0.7)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 0 -7.635 270)
		(size 0.27 1.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.1) (xy -0.465 0.1) (xy -0.465 -0.1) (xy 0.035 -0.1)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.7) (xy -0.465 -0.7) (xy -0.465 -0.9) (xy 0.035 -0.9)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 -0.3)
				(mid -0.093579 -0.158579)
				(end -0.235 -0.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.7)
				(mid -0.093579 -0.641421)
				(end -0.035 -0.5)
				(width 0.2)
			)
			(gr_poly
				(pts
					(xy 0.035 0.9) (xy -0.465 0.9) (xy -0.465 0.7) (xy 0.035 0.7)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.235 0.1)
				(mid -0.093579 0.158579)
				(end -0.035 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.035 0.5)
				(mid -0.093579 0.641421)
				(end -0.235 0.7)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 0.8 7.635 90)
		(size 0.27 1.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.1) (xy -0.465 0.1) (xy -0.465 -0.1) (xy 0.035 -0.1)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.7) (xy -0.465 -0.7) (xy -0.465 -0.9) (xy 0.035 -0.9)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 -0.3)
				(mid -0.093579 -0.158579)
				(end -0.235 -0.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.7)
				(mid -0.093579 -0.641421)
				(end -0.035 -0.5)
				(width 0.2)
			)
			(gr_poly
				(pts
					(xy 0.035 0.9) (xy -0.465 0.9) (xy -0.465 0.7) (xy 0.035 0.7)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.235 0.1)
				(mid -0.093579 0.158579)
				(end -0.035 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.035 0.5)
				(mid -0.093579 0.641421)
				(end -0.235 0.7)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.4 -7.635 270)
		(size 0.27 1.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.1) (xy -0.465 0.1) (xy -0.465 -0.1) (xy 0.035 -0.1)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.7) (xy -0.465 -0.7) (xy -0.465 -0.9) (xy 0.035 -0.9)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 -0.3)
				(mid -0.093579 -0.158579)
				(end -0.235 -0.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.7)
				(mid -0.093579 -0.641421)
				(end -0.035 -0.5)
				(width 0.2)
			)
			(gr_poly
				(pts
					(xy 0.035 0.9) (xy -0.465 0.9) (xy -0.465 0.7) (xy 0.035 0.7)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.235 0.1)
				(mid -0.093579 0.158579)
				(end -0.035 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.035 0.5)
				(mid -0.093579 0.641421)
				(end -0.235 0.7)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.285 -7.185 180)
		(size 0.87 0.87)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.385 0.375) (xy -0.385 0.375) (xy -0.385 -0.285) (xy -0.81 -0.285) (xy -0.81 -0.485) (xy 0.385 -0.485)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.585 -0.285)
				(mid -0.443579 -0.226421)
				(end -0.385 -0.085)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.285 -7.185 180)
		(size 0.87 1.07)
		(layers "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.385 0.485) (xy -0.385 0.485) (xy -0.385 -0.285) (xy -0.81 -0.285) (xy -0.81 -0.485) (xy 0.385 -0.485)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.585 -0.285)
				(mid -0.443579 -0.226421)
				(end -0.385 -0.085)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.285 7.185 180)
		(size 0.87 0.87)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.385 0.485) (xy -0.81 0.485) (xy -0.81 0.285) (xy -0.385 0.285) (xy -0.385 -0.375) (xy 0.385 -0.375)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.385 0.085)
				(mid -0.443579 0.226421)
				(end -0.585 0.285)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.285 7.185 180)
		(size 0.87 1.07)
		(layers "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.385 0.485) (xy -0.81 0.485) (xy -0.81 0.285) (xy -0.385 0.285) (xy -0.385 -0.485) (xy 0.385 -0.485)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.385 0.085)
				(mid -0.443579 0.226421)
				(end -0.585 0.285)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.635 -5.6 180)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.635 -4 180)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.635 -2.4 180)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.635 -0.8 180)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.635 1.6 180)
		(size 0.27 1.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.1) (xy -0.465 0.1) (xy -0.465 -0.1) (xy 0.035 -0.1)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.7) (xy -0.465 -0.7) (xy -0.465 -0.9) (xy 0.035 -0.9)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 -0.3)
				(mid -0.093579 -0.158579)
				(end -0.235 -0.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.7)
				(mid -0.093579 -0.641421)
				(end -0.035 -0.5)
				(width 0.2)
			)
			(gr_poly
				(pts
					(xy 0.035 0.9) (xy -0.465 0.9) (xy -0.465 0.7) (xy 0.035 0.7)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.235 0.1)
				(mid -0.093579 0.158579)
				(end -0.035 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.035 0.5)
				(mid -0.093579 0.641421)
				(end -0.235 0.7)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 4.635 3.8 180)
		(size 0.27 0.6)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.035 0.5) (xy -0.465 0.5) (xy -0.465 0.3) (xy 0.035 0.3)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.035 -0.3) (xy -0.465 -0.3) (xy -0.465 -0.5) (xy 0.035 -0.5)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_arc
				(start -0.035 0.1)
				(mid -0.093579 0.241421)
				(end -0.235 0.3)
				(width 0.2)
			)
			(gr_arc
				(start -0.235 -0.3)
				(mid -0.093579 -0.241421)
				(end -0.035 -0.1)
				(width 0.2)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.5 -7.185)
		(size 1.5 1.27)
		(layers "F.Cu")
		(roundrect_rratio 0.079)
		(zone_connect 0)
	)
	(pad "2" smd roundrect
		(at -4.85 -5.6)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "3" smd roundrect
		(at -4.85 -4)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "4" smd roundrect
		(at -4.85 -2.4)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "5" smd roundrect
		(at -4.85 -0.8)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "6" smd roundrect
		(at -4.85 1.2)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "7" smd roundrect
		(at -4.85 2.4)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "8" smd roundrect
		(at -4.85 3.4)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "9" smd roundrect
		(at -4.85 4.2)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "10" smd roundrect
		(at -4.85 5.6)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "11" smd roundrect
		(at -4.5 7.185)
		(size 1.5 1.27)
		(layers "F.Cu")
		(roundrect_rratio 0.079)
		(zone_connect 0)
	)
	(pad "12" smd roundrect
		(at -3.2 7.85 90)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "13" smd roundrect
		(at -2.4 7.85 90)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "14" smd roundrect
		(at -1.6 7.85 90)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "15" smd roundrect
		(at -0.8 7.85 90)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "16" smd roundrect
		(at 0.8 7.85 90)
		(size 0.8 2.1)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "17" smd roundrect
		(at 2.4 7.85 90)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "18" smd roundrect
		(at 3.2 7.85 90)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "19" smd roundrect
		(at 4.5 7.185 180)
		(size 1.5 1.27)
		(layers "F.Cu")
		(roundrect_rratio 0.079)
		(zone_connect 0)
	)
	(pad "20" smd roundrect
		(at 4.85 6)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "21" smd roundrect
		(at 4.85 5.2)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.05)
	)
	(pad "22" smd roundrect
		(at 4.85 3.8 180)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "23" smd roundrect
		(at 4.85 1.6 180)
		(size 0.8 2.1)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "24" smd roundrect
		(at 4.85 -0.8 180)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "25" smd roundrect
		(at 4.85 -2.4 180)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "26" smd roundrect
		(at 4.85 -4 180)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "27" smd roundrect
		(at 4.85 -5.6 180)
		(size 0.8 1.3)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "28" smd roundrect
		(at 4.5 -7.185 180)
		(size 1.5 1.27)
		(layers "F.Cu")
		(roundrect_rratio 0.079)
		(zone_connect 0)
	)
	(pad "29" smd roundrect
		(at 2.4 -7.85 270)
		(size 0.8 2.1)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "30" smd roundrect
		(at 0 -7.85 270)
		(size 0.8 2.1)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "31" smd roundrect
		(at -2.4 -7.85 270)
		(size 0.8 2.1)
		(layers "F.Cu")
		(roundrect_rratio 0.125)
		(zone_connect 0)
	)
	(pad "32" smd roundrect
		(at -2.4 -5.6)
		(size 1.1 1.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.091)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.07)
	)
	(pad "33" smd roundrect
		(at -2.4 -2.4)
		(size 1.1 1.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.091)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.07)
	)
	(pad "34" smd roundrect
		(at 0 -5.6)
		(size 1.1 1.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.091)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.07)
	)
	(pad "35" smd roundrect
		(at 0 -2.4)
		(size 1.1 1.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.091)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.07)
	)
	(pad "36" smd roundrect
		(at 2.4 -5.6)
		(size 1.1 1.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.091)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.07)
	)
	(pad "37" smd roundrect
		(at 2.4 -2.4)
		(size 1.1 1.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.091)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.07)
	)
	(pad "38" smd roundrect
		(at 3.55 1.6)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.091)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.07)
	)
	(pad "39" smd roundrect
		(at 3.55 3.8)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.091)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.07)
	)
	(pad "40" smd roundrect
		(at 0.335 2.79)
		(size 1.85 2.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.054)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.08)
	)
	(pad "41" smd roundrect
		(at 0.335 5.11)
		(size 1.85 2.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.054)
		(solder_mask_margin -0.05)
		(solder_paste_margin_ratio -0.08)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_QFN-41_10x16mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
