(footprint "Texas_REF0038A_WQFN-38-2EP_6x4mm_P0.4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas REF0038A WQFN, 38 Pin, 2EP (https://www.ti.com/lit/ds/symlink/tps25730.pdf#page=68)")
	(tags "Texas Instruments WQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_REF0038A_WQFN-38-2EP_6x4mm_P0.4"
		(at 0 3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.66 -0.69 180)
		(size 1.17 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.2136752137)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.66 0.69 180)
		(size 1.19 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.2136752137)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.27 -0.69 180)
		(size 1.17 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.2136752137)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.27 0.69 180)
		(size 1.19 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.2136752137)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.56 -0.69 180)
		(size 1.4 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.2136752137)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.56 0.69 180)
		(size 1.4 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.2136752137)
		(thermal_bridge_angle 45)
	)
	(pad "1" smd roundrect
		(at -2.925 -1)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -2.925 -0.6)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -2.925 -0.2)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -2.925 0.2)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -2.925 0.6)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at -2.925 1)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at -2.4 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at -2 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at -1.6 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at -1.2 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at -0.8 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at -0.4 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at 0 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at 0.4 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at 0.8 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd roundrect
		(at 1.2 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd roundrect
		(at 1.6 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd roundrect
		(at 2 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "19" smd roundrect
		(at 2.4 1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "20" smd roundrect
		(at 2.925 0.6625)
		(size 0.65 1.2)
		(layers "F.Cu")
		(roundrect_rratio 0.07692307692)
		(thermal_bridge_angle 45)
	)
	(pad "23" smd roundrect
		(at 2.925 -0.6625)
		(size 0.65 1.2)
		(layers "F.Cu")
		(roundrect_rratio 0.07692307692)
		(thermal_bridge_angle 45)
	)
	(pad "26" smd roundrect
		(at 2.4 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "27" smd roundrect
		(at 2 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "28" smd roundrect
		(at 1.6 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "29" smd roundrect
		(at 1.2 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "30" smd roundrect
		(at 0.8 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "31" smd roundrect
		(at 0.4 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "32" smd roundrect
		(at -0.2 -1.925 90)
		(size 0.6 0.65)
		(layers "F.Cu")
		(roundrect_rratio 0.08333333333)
		(thermal_bridge_angle 45)
	)
	(pad "34" smd roundrect
		(at -1 -1.925 90)
		(size 0.6 0.65)
		(layers "F.Cu")
		(roundrect_rratio 0.08333333333)
		(thermal_bridge_angle 45)
	)
	(pad "36" smd roundrect
		(at -1.6 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "37" smd roundrect
		(at -2 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "38" smd roundrect
		(at -2.4 -1.925 90)
		(size 0.55 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "39" thru_hole circle
		(at -2.075 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at -0.965 -1.075)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at -0.965 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "39" smd roundrect
		(at -0.965 0 180)
		(size 2.72 2.65)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.09433962264)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "39" smd roundrect
		(at -0.965 0 180)
		(size 2.72 2.65)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(roundrect_rratio 0.09433962264)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "39" thru_hole circle
		(at -0.965 1.075)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at 0.145 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "40" thru_hole circle
		(at 1.56 -1.075)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "40" thru_hole circle
		(at 1.56 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "40" smd roundrect
		(at 1.56 0 180)
		(size 1.53 2.65)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1633986928)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "40" smd roundrect
		(at 1.56 0 180)
		(size 1.53 2.65)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(roundrect_rratio 0.1633986928)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "40" thru_hole circle
		(at 1.56 1.075)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_REF0038A_WQFN-38-2EP_6x4mm_P0.4.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
