(footprint "Texas_RGY_R-PVQFN-N20_EP2.05x3.05mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "QFN, 20 Pin, RGY0020A (https://www.ti.com/lit/ds/symlink/txb0108.pdf#page=33)")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_RGY_R-PVQFN-N20_EP2.05x3.05mm"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.56 -0.77)
		(size 0.92 1.33)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.56 0.77)
		(size 0.92 1.33)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 -0.77)
		(size 0.92 1.33)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 0.77)
		(size 0.92 1.33)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -0.75 -2.15 90)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -1.65 -1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -1.65 -1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -1.65 -0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -1.65 -0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at -1.65 0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at -1.65 0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at -1.65 1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at -1.65 1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at -0.75 2.15 90)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at 0.75 2.15 90)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at 1.65 1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at 1.65 1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at 1.65 0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at 1.65 0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd roundrect
		(at 1.65 -0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd roundrect
		(at 1.65 -0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd roundrect
		(at 1.65 -1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "19" smd roundrect
		(at 1.65 -1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "20" smd roundrect
		(at 0.75 -2.15 90)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "21" smd roundrect
		(at 0 0)
		(size 2.05 3.05)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.0243902439)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGY_R-PVQFN-N20_EP2.05x3.05mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
