(footprint "Texas_RGY_R-PVQFN-N24_EP2.05x3.1mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "QFN, 24 Pin (http://www.ti.com/lit/ds/symlink/bq24133.pdf#page=40)")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -4.08 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_RGY_R-PVQFN-N24_EP2.05x3.1mm_ThermalVias"
		(at 0 4.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.56 -0.81)
		(size 0.82 1.32)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.56 0.81)
		(size 0.82 1.32)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 -0.81)
		(size 0.82 1.32)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 0.81)
		(size 0.82 1.32)
		(layers "F.Paste")
	)
	(pad "1" smd custom
		(at -0.75 -2.795)
		(size 0.28 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0 0.3425)
				(end 0.14 0.3425)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at -1.795 -2.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.355 0)
				(end 0.495 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd custom
		(at -1.795 -1.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd custom
		(at -1.795 -1.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd custom
		(at -1.795 -0.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "6" smd custom
		(at -1.795 -0.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "7" smd custom
		(at -1.795 0.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "8" smd custom
		(at -1.795 0.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "9" smd custom
		(at -1.795 1.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "10" smd custom
		(at -1.795 1.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "11" smd custom
		(at -1.795 2.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.3425 0)
				(end 0.4825 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "12" smd custom
		(at -0.75 2.795)
		(size 0.28 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0 -0.3425)
				(end 0.14 -0.3425)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "13" smd custom
		(at 0.75 2.795)
		(size 0.28 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0 -0.3425)
				(end 0.14 -0.3425)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "14" smd custom
		(at 1.795 2.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "15" smd custom
		(at 1.795 1.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "16" smd custom
		(at 1.795 1.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "17" smd custom
		(at 1.795 0.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "18" smd custom
		(at 1.795 0.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "19" smd custom
		(at 1.795 -0.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "20" smd custom
		(at 1.795 -0.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "21" smd custom
		(at 1.795 -1.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "22" smd custom
		(at 1.795 -1.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "23" smd custom
		(at 1.795 -2.25)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.3425 0)
				(end -0.2025 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "24" smd custom
		(at 0.75 -2.795)
		(size 0.28 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0 0.3425)
				(end 0.14 0.3425)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "25" thru_hole circle
		(at -0.5 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -0.5 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -0.5 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" smd rect
		(at 0 0)
		(size 2.05 3.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "25" smd rect
		(at 0 0)
		(size 2.05 3.1)
		(layers "B.Cu")
	)
	(pad "25" thru_hole circle
		(at 0.5 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 0.5 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 0.5 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGY_R-PVQFN-N24_EP2.05x3.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
