(footprint "Texas_RHH0036C_VQFN-36-1EP_6x6mm_P0.5mm_EP4.4x4.4mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas RHH0036C VQFN, 36 Pin (http://www.ti.com/lit/ds/slvsba5d/slvsba5d.pdf#page=37), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "Texas VQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -4.33 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_RHH0036C_VQFN-36-1EP_6x6mm_P0.5mm_EP4.4x4.4mm_ThermalVias"
		(at 0 4.33 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.8875 -1.8875)
		(size 0.389528 0.389528)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.137582 -0.137582)
					(xy 0.137582 -0.137582)
					(xy 0.137582 0.042841)
					(xy 0.042841 0.137582)
					(xy -0.137582 0.137582)
				)
				(width 0.228726)
			)
		)
	)
	(pad "" smd custom
		(at -1.8875 -1.05)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.166699 -0.338022)
					(xy 0.096078 -0.338022)
					(xy 0.166699 -0.267401)
					(xy 0.166699 0.267401)
					(xy 0.096078 0.338022)
					(xy -0.166699 0.338022)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at -1.8875 0)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.166699 -0.338022)
					(xy 0.096078 -0.338022)
					(xy 0.166699 -0.267401)
					(xy 0.166699 0.267401)
					(xy 0.096078 0.338022)
					(xy -0.166699 0.338022)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at -1.8875 1.05)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.166699 -0.338022)
					(xy 0.096078 -0.338022)
					(xy 0.166699 -0.267401)
					(xy 0.166699 0.267401)
					(xy 0.096078 0.338022)
					(xy -0.166699 0.338022)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at -1.8875 1.8875)
		(size 0.389528 0.389528)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.137582 -0.137582)
					(xy 0.042841 -0.137582)
					(xy 0.137582 -0.042841)
					(xy 0.137582 0.137582)
					(xy -0.137582 0.137582)
				)
				(width 0.228726)
			)
		)
	)
	(pad "" smd custom
		(at -1.05 -1.8875)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.338022 -0.166699)
					(xy 0.338022 -0.166699)
					(xy 0.338022 0.096078)
					(xy 0.267401 0.166699)
					(xy -0.267401 0.166699)
					(xy -0.338022 0.096078)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd roundrect
		(at -1.05 -1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.05 0)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.05 1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at -1.05 1.8875)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.338022 -0.096078)
					(xy -0.267401 -0.166699)
					(xy 0.267401 -0.166699)
					(xy 0.338022 -0.096078)
					(xy 0.338022 0.166699)
					(xy -0.338022 0.166699)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at 0 -1.8875)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.338022 -0.166699)
					(xy 0.338022 -0.166699)
					(xy 0.338022 0.096078)
					(xy 0.267401 0.166699)
					(xy -0.267401 0.166699)
					(xy -0.338022 0.096078)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd roundrect
		(at 0 -1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at 0 1.8875)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.338022 -0.096078)
					(xy -0.267401 -0.166699)
					(xy 0.267401 -0.166699)
					(xy 0.338022 -0.096078)
					(xy 0.338022 0.166699)
					(xy -0.338022 0.166699)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at 1.05 -1.8875)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.338022 -0.166699)
					(xy 0.338022 -0.166699)
					(xy 0.338022 0.096078)
					(xy 0.267401 0.166699)
					(xy -0.267401 0.166699)
					(xy -0.338022 0.096078)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd roundrect
		(at 1.05 -1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.05 0)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.05 1.05)
		(size 0.846537 0.846537)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at 1.05 1.8875)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.338022 -0.096078)
					(xy -0.267401 -0.166699)
					(xy 0.267401 -0.166699)
					(xy 0.338022 -0.096078)
					(xy 0.338022 0.166699)
					(xy -0.338022 0.166699)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at 1.8875 -1.8875)
		(size 0.389528 0.389528)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.137582 -0.137582)
					(xy 0.137582 -0.137582)
					(xy 0.137582 0.137582)
					(xy -0.042841 0.137582)
					(xy -0.137582 0.042841)
				)
				(width 0.228726)
			)
		)
	)
	(pad "" smd custom
		(at 1.8875 -1.05)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.166699 -0.267401)
					(xy -0.096078 -0.338022)
					(xy 0.166699 -0.338022)
					(xy 0.166699 0.338022)
					(xy -0.096078 0.338022)
					(xy -0.166699 0.267401)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at 1.8875 0)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.166699 -0.267401)
					(xy -0.096078 -0.338022)
					(xy 0.166699 -0.338022)
					(xy 0.166699 0.338022)
					(xy -0.096078 0.338022)
					(xy -0.166699 0.267401)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at 1.8875 1.05)
		(size 0.418645 0.418645)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.166699 -0.267401)
					(xy -0.096078 -0.338022)
					(xy 0.166699 -0.338022)
					(xy 0.166699 0.338022)
					(xy -0.096078 0.338022)
					(xy -0.166699 0.267401)
				)
				(width 0.170493)
			)
		)
	)
	(pad "" smd custom
		(at 1.8875 1.8875)
		(size 0.389528 0.389528)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.137582 -0.042841)
					(xy -0.042841 -0.137582)
					(xy 0.137582 -0.137582)
					(xy 0.137582 0.137582)
					(xy -0.137582 0.137582)
				)
				(width 0.228726)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.8875 -2)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.8875 -1.5)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.8875 -1)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.8875 -0.5)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.8875 0)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.8875 0.5)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.8875 1)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -2.8875 1.5)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -2.8875 2)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -2 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -1.5 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -1 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -0.5 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 0.5 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.5 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 2 2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 2.8875 2)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.8875 1.5)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.8875 1)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 2.8875 0.5)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 2.8875 0)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.8875 -0.5)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 2.8875 -1)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 2.8875 -1.5)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 2.8875 -2)
		(size 0.975 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 2 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 1.5 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 1 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 0.5 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 0 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at -0.5 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at -1 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at -1.5 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -2 -2.8875)
		(size 0.25 0.975)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" thru_hole circle
		(at -1.575 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -1.575 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -1.575 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -1.575 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -0.525 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -0.525 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -0.525 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -0.525 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" smd rect
		(at 0 0)
		(size 3.65 3.65)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "37" smd rect
		(at 0 0)
		(size 4.4 4.4)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "37" thru_hole circle
		(at 0.525 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 0.525 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 0.525 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 0.525 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 1.575 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 1.575 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 1.575 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 1.575 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RHH0036C_VQFN-36-1EP_6x6mm_P0.5mm_EP4.4x4.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
