(footprint "Texas_RJE0020A_VQFN-20-1EP_3x3mm_P0.45mm_EP0.675x0.76mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas RJE0020A VQFN, 20 Pin (https://www.ti.com/lit/ds/symlink/tps51396a.pdf#page=31), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "Texas VQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_RJE0020A_VQFN-20-1EP_3x3mm_P0.45mm_EP0.675x0.76mm"
		(at 0 2.83 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.06 -0.018)
		(size 0.64 0.72)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd custom
		(at -1.4375 -0.9)
		(size 0.072721 0.072721)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4275 -0.09)
					(xy 0.253358 -0.09)
					(xy 0.4275 0.084142)
					(xy 0.4275 0.09)
					(xy -0.4275 0.09)
				)
				(width 0.02)
			)
		)
	)
	(pad "2" smd roundrect
		(at -1.4375 -0.45)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.4375 0)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.4375 0.45)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at -1.4375 0.9)
		(size 0.072721 0.072721)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4275 -0.09)
					(xy 0.4275 -0.09)
					(xy 0.4275 -0.084142)
					(xy 0.253358 0.09)
					(xy -0.4275 0.09)
				)
				(width 0.02)
			)
		)
	)
	(pad "6" smd custom
		(at -0.9 1.4375)
		(size 0.072721 0.072721)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.09 -0.253358)
					(xy 0.084142 -0.4275)
					(xy 0.09 -0.4275)
					(xy 0.09 0.4275)
					(xy -0.09 0.4275)
				)
				(width 0.02)
			)
		)
	)
	(pad "7" smd roundrect
		(at -0.45 1.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0 1.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.45 1.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd custom
		(at 0.9 1.4375)
		(size 0.072721 0.072721)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.09 -0.4275)
					(xy -0.084142 -0.4275)
					(xy 0.09 -0.253358)
					(xy 0.09 0.4275)
					(xy -0.09 0.4275)
				)
				(width 0.02)
			)
		)
	)
	(pad "11" smd custom
		(at 1.4375 0.9)
		(size 0.072721 0.072721)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4275 -0.09)
					(xy 0.4275 -0.09)
					(xy 0.4275 0.09)
					(xy -0.253358 0.09)
					(xy -0.4275 -0.084142)
				)
				(width 0.02)
			)
		)
	)
	(pad "12" smd roundrect
		(at 1.4375 0.45)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.4375 0)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.4375 -0.45)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd custom
		(at 1.4375 -0.9)
		(size 0.072721 0.072721)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4275 0.084142)
					(xy -0.253358 -0.09)
					(xy 0.4275 -0.09)
					(xy 0.4275 0.09)
					(xy -0.4275 0.09)
				)
				(width 0.02)
			)
		)
	)
	(pad "16" smd custom
		(at 0.9 -1.4375)
		(size 0.072721 0.072721)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.09 -0.4275)
					(xy 0.09 -0.4275)
					(xy 0.09 0.253358)
					(xy -0.084142 0.4275)
					(xy -0.09 0.4275)
				)
				(width 0.02)
			)
		)
	)
	(pad "17" smd roundrect
		(at 0.45 -1.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 0 -1.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -0.45 -1.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd custom
		(at -0.9 -1.4375)
		(size 0.072721 0.072721)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.09 -0.4275)
					(xy 0.09 -0.4275)
					(xy 0.09 0.4275)
					(xy 0.084142 0.4275)
					(xy -0.09 0.253358)
				)
				(width 0.02)
			)
		)
	)
	(pad "21" smd rect
		(at -0.06 -0.018)
		(size 0.675 0.76)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RJE0020A_VQFN-20-1EP_3x3mm_P0.45mm_EP0.675x0.76mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
