(footprint "Texas_RNN0018A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Instruments, VQFN-HR RNN0018A (http://www.ti.com/lit/ds/symlink/tps568215.pdf)")
	(tags "ti vqfn-hr rnn0018a")
	(property "Reference" "REF**"
		(at 0 -3.175 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_RNN0018A"
		(at 0 3.175 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.375 -0.35)
		(size 1.15 0.36)
		(layers "F.Paste")
		(roundrect_rratio 0.139)
	)
	(pad "" smd roundrect
		(at -0.3 -0.2825)
		(size 0.3 0.733)
		(layers "F.Paste")
		(roundrect_rratio 0.167)
	)
	(pad "" smd roundrect
		(at -0.3 0.651)
		(size 0.3 0.733)
		(layers "F.Paste")
		(roundrect_rratio 0.167)
	)
	(pad "" smd roundrect
		(at -0.3 1.585)
		(size 0.3 0.733)
		(layers "F.Paste")
		(roundrect_rratio 0.167)
	)
	(pad "" smd roundrect
		(at 0.3 -0.2825)
		(size 0.3 0.733)
		(layers "F.Paste")
		(roundrect_rratio 0.167)
	)
	(pad "" smd roundrect
		(at 0.3 0.651)
		(size 0.3 0.733)
		(layers "F.Paste")
		(roundrect_rratio 0.167)
	)
	(pad "" smd roundrect
		(at 0.3 1.585)
		(size 0.3 0.733)
		(layers "F.Paste")
		(roundrect_rratio 0.167)
	)
	(pad "" smd roundrect
		(at 1.375 -0.35)
		(size 1.15 0.36)
		(layers "F.Paste")
		(roundrect_rratio 0.139)
	)
	(pad "1" smd roundrect
		(at -1.65 -0.925)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "2" smd roundrect
		(at -1.375 -0.35)
		(size 1.15 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "3" smd roundrect
		(at -1.375 0.3)
		(size 1.15 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "4" smd roundrect
		(at -1.375 0.85)
		(size 1.15 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "5" smd roundrect
		(at -1.375 1.4)
		(size 1.15 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "6" smd roundrect
		(at -0.3 0.65)
		(size 0.3 2.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.166)
	)
	(pad "7" smd roundrect
		(at 0.3 0.65)
		(size 0.3 2.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.166)
	)
	(pad "8" smd roundrect
		(at 1.375 1.4)
		(size 1.15 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "9" smd roundrect
		(at 1.375 0.85)
		(size 1.15 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "10" smd roundrect
		(at 1.375 0.3)
		(size 1.15 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "11" smd roundrect
		(at 1.375 -0.35)
		(size 1.15 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "12" smd roundrect
		(at 1.65 -0.925)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "13" smd roundrect
		(at 1.25 -1.65)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "14" smd roundrect
		(at 0.75 -1.65)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "15" smd roundrect
		(at 0.25 -1.65)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "16" smd roundrect
		(at -0.25 -1.65)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "17" smd roundrect
		(at -0.75 -1.65)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "18" smd roundrect
		(at -1.25 -1.65)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RNN0018A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
