(footprint "Texas_RPU0010A_VQFN-HR-10_2x2mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "VQFN-HR, 10 Pin (https://www.ti.com/lit/ds/symlink/tps62912.pdf#page=39)")
	(tags "VQFN-HR NO LEAD")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_RPU0010A_VQFN-HR-10_2x2mm_P0.5mm"
		(at 0 2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.875 -0.25)
		(size 0.65 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -0.7 0.25)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -0.875 0.75)
		(size 0.65 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 0.7 0.75)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at 0.875 0.25)
		(size 0.65 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at 0.7 -0.25)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at 0.75 -0.925)
		(size 0.25 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 0.25 -0.925)
		(size 0.25 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at -0.25 -0.925)
		(size 0.25 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at -0.75 -0.925)
		(size 0.25 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RPU0010A_VQFN-HR-10_2x2mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
