(footprint "Texas_RSN_WQFN-32-1EP_4x4mm_P0.4mm_EP2.8x2.8mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas RSN WQFN, 32 Pin (https://www.ti.com/lit/ds/symlink/bq25703a.pdf#page=90), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "Texas WQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.33 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_RSN_WQFN-32-1EP_4x4mm_P0.4mm_EP2.8x2.8mm_ThermalVias"
		(at 0 3.33 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.7 -0.7)
		(size 1.17 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.213675)
	)
	(pad "" smd roundrect
		(at -0.7 0.7)
		(size 1.17 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.213675)
	)
	(pad "" smd roundrect
		(at 0.7 -0.7)
		(size 1.17 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.213675)
	)
	(pad "" smd roundrect
		(at 0.7 0.7)
		(size 1.17 1.17)
		(layers "F.Paste")
		(roundrect_rratio 0.213675)
	)
	(pad "1" smd roundrect
		(at -1.9875 -1.4)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.9875 -1)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.9875 -0.6)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.9875 -0.2)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.9875 0.2)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.9875 0.6)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.9875 1)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -1.9875 1.4)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -1.4 1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -1 1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -0.6 1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -0.2 1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.2 1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.6 1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1 1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1.4 1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.9875 1.4)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.9875 1)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.9875 0.6)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.9875 0.2)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 1.9875 -0.2)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.9875 -0.6)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1.9875 -1)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 1.9875 -1.4)
		(size 0.775 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 1.4 -1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 1 -1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 0.6 -1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 0.2 -1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -0.2 -1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -0.6 -1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -1 -1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -1.4 -1.9875)
		(size 0.2 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" thru_hole circle
		(at -1.1 -1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -1.1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -1.1 1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0 -1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 2.8 2.8)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 2.8 2.8)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "33" thru_hole circle
		(at 0 1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.1 -1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.1 1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RSN_WQFN-32-1EP_4x4mm_P0.4mm_EP2.8x2.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
