(footprint "Texas_RWH0032A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Instruments, RWH0032A, 8x8x0.9mm (http://www.ti.com/lit/ds/snosd10c/snosd10c.pdf)")
	(tags "ti rwh0032a")
	(property "Reference" "REF**"
		(at 0 -5.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_RWH0032A"
		(at 0 5.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin -0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -3.8 -2.6)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.8 -1.95)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.8 -1.3)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.8 -0.65)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.8 0)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.8 0.65)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.8 1.3)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.8 1.95)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.8 2.6)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 0.05 -3.8)
		(size 0.6 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "" smd roundrect
		(at 0.05 3.8)
		(size 0.6 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "" smd roundrect
		(at 0.325 -2.38)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 0.325 -1.19)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 0.325 0)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 0.325 1.19)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 0.325 2.38)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 0.8 -3.8)
		(size 0.4 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 0.8 3.8)
		(size 0.4 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 1.45 -3.8)
		(size 0.4 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 1.45 3.8)
		(size 0.4 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 2.1 -3.8)
		(size 0.4 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 2.1 3.8)
		(size 0.4 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 2.125 -2.38)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 2.125 -1.19)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 2.125 0)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 2.125 1.19)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 2.125 2.38)
		(size 1.6 0.99)
		(layers "F.Paste")
		(roundrect_rratio 0.051)
	)
	(pad "" smd roundrect
		(at 2.9 -3.8)
		(size 0.6 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "" smd roundrect
		(at 2.9 3.8)
		(size 0.6 0.76)
		(layers "F.Paste")
		(roundrect_rratio 0.084)
	)
	(pad "" smd roundrect
		(at 3.8 -2.6)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.8 -1.95)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.8 -1.3)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.8 -0.65)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.8 0)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.8 0.65)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.8 1.3)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.8 1.95)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.8 2.6)
		(size 0.76 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "1" smd roundrect
		(at -3.8 -3.45)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.055)
		(solder_paste_margin -0.07)
	)
	(pad "2" smd roundrect
		(at -3.8 -2.6)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -3.8 -1.95)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -3.8 -1.3)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "5" smd roundrect
		(at -3.8 -0.65)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -3.8 0)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "7" smd roundrect
		(at -3.8 0.65)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "8" smd roundrect
		(at -3.8 1.3)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "9" smd roundrect
		(at -3.8 1.95)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "10" smd roundrect
		(at -3.8 2.6)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "11" smd roundrect
		(at -3.8 3.45)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.055)
		(solder_paste_margin -0.07)
	)
	(pad "12" smd roundrect
		(at 0.05 3.8)
		(size 0.7 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.072)
	)
	(pad "13" smd roundrect
		(at 0.8 3.8)
		(size 0.5 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "14" smd roundrect
		(at 1.45 3.8)
		(size 0.5 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "15" smd roundrect
		(at 2.1 3.8)
		(size 0.5 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "16" smd roundrect
		(at 2.9 3.8)
		(size 0.7 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.072)
	)
	(pad "17" smd roundrect
		(at 3.8 3.45)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.055)
		(solder_paste_margin -0.07)
	)
	(pad "18" smd roundrect
		(at 3.8 2.6)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "19" smd roundrect
		(at 3.8 1.95)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "20" smd roundrect
		(at 3.8 1.3)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "21" smd roundrect
		(at 3.8 0.65)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "22" smd roundrect
		(at 3.8 0)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "23" smd roundrect
		(at 3.8 -0.65)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "24" smd roundrect
		(at 3.8 -1.3)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "25" smd roundrect
		(at 3.8 -1.95)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "26" smd roundrect
		(at 3.8 -2.6)
		(size 0.9 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "27" smd roundrect
		(at 3.8 -3.45)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.055)
		(solder_paste_margin -0.07)
	)
	(pad "28" smd roundrect
		(at 2.9 -3.8)
		(size 0.7 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.072)
	)
	(pad "29" smd roundrect
		(at 2.1 -3.8)
		(size 0.5 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "30" smd roundrect
		(at 1.45 -3.8)
		(size 0.5 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "31" smd roundrect
		(at 0.8 -3.8)
		(size 0.5 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "32" smd roundrect
		(at 0.05 -3.8)
		(size 0.7 0.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.072)
	)
	(pad "33" smd roundrect
		(at 1.225 0)
		(size 3.85 6.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.013)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RWH0032A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
