(footprint "Texas_S-PVQFN-N14"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas_S-PVQFN-N14  http://www.ti.com/lit/ds/symlink/txb0104.pdf")
	(tags "Texas_S-PVQFN-N14_4.3x4.3_Pitch0.5mm_ThermalPad")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_S-PVQFN-N14"
		(at 0 3.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.56 -0.56 270)
		(size 0.82 0.82)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.56 0.56 270)
		(size 0.82 0.82)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 -0.56 270)
		(size 0.82 0.82)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 0.56 270)
		(size 0.82 0.82)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -0.75 -1.725 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.725 -1 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.725 -0.5 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.725 0 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.725 0.5 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.725 1 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.75 1.725 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.75 1.725 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.725 1 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.725 0.5 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.725 0 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.725 -0.5 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.725 -1 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 0.75 -1.725 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0 0 270)
		(size 2.05 2.05)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N14.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
