(footprint "Texas_S-PWQFN-N100_EP5.5x5.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.ti.com/general/docs/lit/getliterature.tsp?baseLiteratureNumber=szza059&fileType=pdf,http://www.ti.com/lit/ds/sllse76m/sllse76m.pdf")
	(tags "MultiRow QFN")
	(property "Reference" "REF**"
		(at 0 -5.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_S-PWQFN-N100_EP5.5x5.5mm"
		(at 0 6.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.66 -1.66)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.66 0)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.66 1.66)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -1.66)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 1.66)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.66 -1.66)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.66 0)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.66 1.66)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "A1" smd rect
		(at -4.4 -3.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at -4.4 -3 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at -4.4 -2.4 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at -4.4 -1.8 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at -4.4 -1.2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at -4.4 -0.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at -4.4 0 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at -4.4 0.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at -4.4 1.2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at -4.4 1.8 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at -4.4 2.4 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at -4.4 3 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd rect
		(at -4.4 3.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd rect
		(at -3.6 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd rect
		(at -3 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd rect
		(at -2.4 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd rect
		(at -1.8 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd rect
		(at -1.2 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd rect
		(at -0.6 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd rect
		(at 0 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd rect
		(at 0.6 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd rect
		(at 1.2 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd rect
		(at 1.8 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A24" smd rect
		(at 2.4 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A25" smd rect
		(at 3 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A26" smd rect
		(at 3.6 4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A27" smd rect
		(at 4.4 3.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A28" smd rect
		(at 4.4 3 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A29" smd rect
		(at 4.4 2.4 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A30" smd rect
		(at 4.4 1.8 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A31" smd rect
		(at 4.4 1.2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A32" smd rect
		(at 4.4 0.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A33" smd rect
		(at 4.4 0 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A34" smd rect
		(at 4.4 -0.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A35" smd rect
		(at 4.4 -1.2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A36" smd rect
		(at 4.4 -1.8 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A37" smd rect
		(at 4.4 -2.4 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A38" smd rect
		(at 4.4 -3 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A39" smd rect
		(at 4.4 -3.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A40" smd rect
		(at 3.6 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A41" smd rect
		(at 3 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A42" smd rect
		(at 2.4 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A43" smd rect
		(at 1.8 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A44" smd rect
		(at 1.2 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A45" smd rect
		(at 0.6 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A46" smd rect
		(at 0 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A47" smd rect
		(at -0.6 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A48" smd rect
		(at -1.2 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A49" smd rect
		(at -1.8 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A50" smd rect
		(at -2.4 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A51" smd rect
		(at -3 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A52" smd rect
		(at -3.6 -4.4)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A53" smd rect
		(at 0 0)
		(size 5.5 5.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B1" smd rect
		(at -3.65 -3.025 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd rect
		(at -3.65 -2.475 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd rect
		(at -3.65 -1.925 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd rect
		(at -3.65 -1.375 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd rect
		(at -3.65 -0.825 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd rect
		(at -3.65 -0.275 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd rect
		(at -3.65 0.275 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd rect
		(at -3.65 0.825 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd rect
		(at -3.65 1.375 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd rect
		(at -3.65 1.925 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd rect
		(at -3.65 2.475 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd rect
		(at -3.65 3.025 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd rect
		(at -3.025 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd rect
		(at -2.475 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd rect
		(at -1.925 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd rect
		(at -1.375 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd rect
		(at -0.825 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd rect
		(at -0.275 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd rect
		(at 0.275 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd rect
		(at 0.825 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B21" smd rect
		(at 1.375 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B22" smd rect
		(at 1.925 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B23" smd rect
		(at 2.475 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B24" smd rect
		(at 3.025 3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B25" smd rect
		(at 3.65 3.025 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B26" smd rect
		(at 3.65 2.475 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B27" smd rect
		(at 3.65 1.925 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B28" smd rect
		(at 3.65 1.375 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B29" smd rect
		(at 3.65 0.825 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B30" smd rect
		(at 3.65 0.275 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B31" smd rect
		(at 3.65 -0.275 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B32" smd rect
		(at 3.65 -0.825 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B33" smd rect
		(at 3.65 -1.375 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B34" smd rect
		(at 3.65 -1.925 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B35" smd rect
		(at 3.65 -2.475 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B36" smd rect
		(at 3.65 -3.025 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B37" smd rect
		(at 3.025 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B38" smd rect
		(at 2.475 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B39" smd rect
		(at 1.925 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B40" smd rect
		(at 1.375 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B41" smd rect
		(at 0.825 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B42" smd rect
		(at 0.275 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B43" smd rect
		(at -0.275 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B44" smd rect
		(at -0.825 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B45" smd rect
		(at -1.375 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B46" smd rect
		(at -1.925 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B47" smd rect
		(at -2.475 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B48" smd rect
		(at -3.025 -3.65)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd rect
		(at -4.25 -4.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd rect
		(at -4.25 4.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd rect
		(at 4.25 4.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd rect
		(at 4.25 -4.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_S-PWQFN-N100_EP5.5x5.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
