(footprint "Texas_S-PWQFN-N20"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "20-Pin Plastic Quad Flatpack No-Lead Package, Body 3.0x3.0x0.8mm, Texas Instruments (http://www.ti.com/lit/ds/symlink/tps22993.pdf)")
	(tags "QFN 0.4")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_S-PWQFN-N20"
		(at 0 2.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.2875 -1.2875)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.2875 1.2875)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.2875 -1.2875)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.2875 1.2875)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd oval
		(at -1.4 -0.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -1.4 -0.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -1.4 0 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -1.4 0.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -1.4 0.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -0.8 1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -0.4 1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 0 1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at 0.4 1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at 0.8 1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at 1.4 0.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at 1.4 0.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at 1.4 0 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 1.4 -0.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at 1.4 -0.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at 0.8 -1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at 0.4 -1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at 0 -1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at -0.4 -1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at -0.8 -1.4)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_S-PWQFN-N20.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
