(footprint "Texas_VQFN-RHL-20"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.ti.com/lit/ds/symlink/bq51050b.pdf")
	(tags "RHL0020A")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_VQFN-RHL-20"
		(at 0 3.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.56 -1.05)
		(size 0.92 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.56 0)
		(size 0.92 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.56 1.05)
		(size 0.92 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -1.8)
		(size 0.75 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 1.8)
		(size 0.75 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 -1.05)
		(size 0.92 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 0)
		(size 0.92 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.56 1.05)
		(size 0.92 0.85)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -0.75 -2.15)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "2" smd roundrect
		(at -1.65 -1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "3" smd roundrect
		(at -1.65 -1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "4" smd roundrect
		(at -1.65 -0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "5" smd roundrect
		(at -1.65 -0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "6" smd roundrect
		(at -1.65 0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "7" smd roundrect
		(at -1.65 0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "8" smd roundrect
		(at -1.65 1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "9" smd roundrect
		(at -1.65 1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "10" smd roundrect
		(at -0.75 2.15)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "11" smd roundrect
		(at 0.75 2.15)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "12" smd roundrect
		(at 1.65 1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "13" smd roundrect
		(at 1.65 1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "14" smd roundrect
		(at 1.65 0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "15" smd roundrect
		(at 1.65 0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "16" smd roundrect
		(at 1.65 -0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "17" smd roundrect
		(at 1.65 -0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "18" smd roundrect
		(at 1.65 -1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "19" smd roundrect
		(at 1.65 -1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "20" smd roundrect
		(at 0.75 -2.15)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.21)
	)
	(pad "21" smd roundrect
		(at -0.275 -2.15)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -0.275 2.15)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd custom
		(at 0 0)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.375 -1.525) (xy 1.025 -1.525) (xy 1.025 1.525) (xy 0.375 1.525) (xy 0.375 1.925) (xy -0.375 1.925)
					(xy -0.375 1.525) (xy -1.025 1.525) (xy -1.025 -1.525) (xy -0.375 -1.525) (xy -0.375 -1.925) (xy 0.375 -1.925)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "21" smd roundrect
		(at 0.275 -2.15)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 0.275 2.15)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_VQFN-RHL-20_ThermalVias.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
