(footprint "Texas_VQFN-RNR0011A-11"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "RNR0011A, VQFN-11 (https://www.ti.com/lit/ds/symlink/tps61089.pdf#Page=27)")
	(tags "TI RNR0011A")
	(property "Reference" "REF**"
		(at 0 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_VQFN-RNR0011A-11"
		(at 0 2.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.375 -1.06)
		(size 0.25 0.28)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(solder_paste_margin 0.05)
	)
	(pad "" smd roundrect
		(at -0.375 -0.7)
		(size 0.25 1)
		(layers "F.Mask")
		(roundrect_rratio 0.15)
	)
	(pad "" smd roundrect
		(at -0.35 0.74)
		(size 0.35 0.92)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(solder_paste_margin 0.05)
	)
	(pad "" smd roundrect
		(at 0 -0.51)
		(size 1 0.62)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 0 -0.46)
		(size 1 0.52)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(solder_paste_margin 0.05)
	)
	(pad "" smd roundrect
		(at 0.35 0.74)
		(size 0.35 0.92)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(solder_paste_margin 0.05)
	)
	(pad "" smd roundrect
		(at 0.375 -1.06)
		(size 0.25 0.28)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(solder_paste_margin 0.05)
	)
	(pad "" smd roundrect
		(at 0.375 -0.7)
		(size 0.25 1)
		(layers "F.Mask")
		(roundrect_rratio 0.15)
	)
	(pad "1" smd roundrect
		(at -1.175 -0.75)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.175 -0.25)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.175 0.25)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.175 0.75)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.35 0.7)
		(size 0.45 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.12)
		(solder_mask_margin -0.05)
	)
	(pad "6" smd roundrect
		(at 0.35 0.7)
		(size 0.45 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.12)
		(solder_mask_margin -0.05)
	)
	(pad "7" smd roundrect
		(at 1.175 0.75 180)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.175 0.25 180)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.175 -0.25 180)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.175 -0.75 180)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" thru_hole circle
		(at 0 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "11" smd roundrect
		(at 0 -0.7)
		(size 1.1 1.1)
		(layers "F.Cu")
		(roundrect_rratio 0.05)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_VQFN-RNR0011A-11.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
