(footprint "UDFN-10_1.35x2.6mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.st.com/content/ccc/resource/technical/document/datasheet/f2/11/8a/ed/40/31/40/56/DM00088292.pdf/files/DM00088292.pdf/jcr:content/translations/en.DM00088292.pdf")
	(tags "UDFN 0.5 uQFN")
	(property "Reference" "REF**"
		(at 0 -2.17 0)
		(layer "F.SilkS")
	)
	(property "Value" "UDFN-10_1.35x2.6mm_P0.5mm"
		(at 0 2.29 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -0.525 -1)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -0.525 -0.5)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -0.525 0)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -0.525 0.5)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -0.525 1)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at 0.525 1)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at 0.525 0.5)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 0.525 0)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at 0.525 -0.5)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at 0.525 -1)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UDFN-10_1.35x2.6mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
