(footprint "UDFN-4-1EP_1x1mm_P0.65mm_EP0.48x0.48mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "UDFN-4_1x1mm_P0.65mm, http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550x-300mA-Single-Output-LDO-in-Small-Packages-DS20006006A.pdf")
	(tags "UDFN-4_1x1mm_P0.65mm")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "UDFN-4-1EP_1x1mm_P0.65mm_EP0.48x0.48mm"
		(at 0 1.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -1.25 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -0.54 -0.325)
		(size 0.22 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.11 0.125) (xy 0.11 -0.125) (xy 0.36 -0.125)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at -0.54 0.325)
		(size 0.22 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.29 0.055) (xy 0.29 0.125) (xy 0.11 0.125) (xy 0.11 -0.125)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd custom
		(at 0.54 0.325)
		(size 0.22 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.11 0.125) (xy -0.29 0.125) (xy -0.29 0.055) (xy -0.11 -0.125)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd custom
		(at 0.54 -0.325)
		(size 0.22 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.11 0.125) (xy -0.29 -0.055) (xy -0.29 -0.125) (xy -0.11 -0.125)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd rect
		(at 0 0 45)
		(size 0.48 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UDFN-4-1EP_1x1mm_P0.65mm_EP0.48x0.48mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
