(footprint "UDFN-9_1.0x3.8mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "9-pin UDFN package, 1.0x3.8mm, (Ref: https://katalog.we-online.de/pbs/datasheet/824014881.pdf)")
	(tags "UDFN SMD")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "UDFN-9_1.0x3.8mm_P0.5mm"
		(at 0 2.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.475 -1.7)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.475 -0.8)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.475 0)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.475 0.8)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.475 1.7)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.475 1.3)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.475 0.4)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.475 -0.4)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.475 -1.3)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UDFN-9_1.0x3.8mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
