(footprint "UQFN-10_1.6x2.1mm_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "UQFN, 10 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/00001725D.pdf (Page 12)), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "UQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "UQFN-10_1.6x2.1mm_P0.5mm"
		(at 0 2.35 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.675 -0.25)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.675 0.25)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.5 1)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0 1)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.5 1)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.675 0.25)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.675 -0.25)
		(size 0.95 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.5 -1)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0 -1)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.5 -1)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UQFN-10_1.6x2.1mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
