(footprint "UQFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16-Lead Ultra Thin Quad Flat, No Lead Package (UC) - 3x3x0.5 mm Body [UQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "QFN 0.5")
	(property "Reference" "REF**"
		(at 0 -2.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "UQFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm"
		(at 0 2.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.4375 -0.4375)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.4375 0.4375)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4375 -0.4375)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4375 0.4375)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "1" smd oval
		(at -1.5 -0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -1.5 -0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -1.5 0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -1.5 0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -0.75 1.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -0.25 1.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at 0.25 1.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 0.75 1.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at 1.5 0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at 1.5 0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at 1.5 -0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at 1.5 -0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at 0.75 -1.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 0.25 -1.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -0.25 -1.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -0.75 -1.5 90)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 0 0)
		(size 1.75 1.75)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UQFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
