(footprint "UQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16-Lead Ultra Thin Plastic Quad Flat, No Lead Package (JQ) - 4x4x0.5 mm Body [UQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "QFN 0.65")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "UQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.675 -0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.675 0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.675 -0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.675 0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
	)
	(pad "1" smd oval
		(at -2 -0.975)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -2 -0.325)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -2 0.325)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -2 0.975)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -0.975 2 90)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -0.325 2 90)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at 0.325 2 90)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 0.975 2 90)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at 2 0.975)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at 2 0.325)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at 2 -0.325)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at 2 -0.975)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at 0.975 -2 90)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 0.325 -2 90)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -0.325 -2 90)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -0.975 -2 90)
		(size 0.8 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 0 0)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
