(footprint "UQFN-20_3x3mm_P0.4mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "UQFN, 20 Pin (https://resurgentsemi.com/wp-content/uploads/2018/09/MPR121_rev5-Resurgent.pdf?d453f8&d453f8), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "UQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "UQFN-20_3x3mm_P0.4mm"
		(at 0 2.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -1.3875 -0.8)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4225 -0.06)
					(xy 0.325931 -0.06)
					(xy 0.4225 0.036569)
					(xy 0.4225 0.06)
					(xy -0.4225 0.06)
				)
				(width 0.08)
			)
		)
	)
	(pad "2" smd roundrect
		(at -1.3875 -0.4)
		(size 0.925 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.3875 0)
		(size 0.925 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.3875 0.4)
		(size 0.925 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at -1.3875 0.8)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4225 -0.06)
					(xy 0.4225 -0.06)
					(xy 0.4225 -0.036569)
					(xy 0.325931 0.06)
					(xy -0.4225 0.06)
				)
				(width 0.08)
			)
		)
	)
	(pad "6" smd custom
		(at -0.8 1.3875)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.06 -0.325931)
					(xy 0.036569 -0.4225)
					(xy 0.06 -0.4225)
					(xy 0.06 0.4225)
					(xy -0.06 0.4225)
				)
				(width 0.08)
			)
		)
	)
	(pad "7" smd roundrect
		(at -0.4 1.3875)
		(size 0.2 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0 1.3875)
		(size 0.2 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.4 1.3875)
		(size 0.2 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd custom
		(at 0.8 1.3875)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.06 -0.4225)
					(xy -0.036569 -0.4225)
					(xy 0.06 -0.325931)
					(xy 0.06 0.4225)
					(xy -0.06 0.4225)
				)
				(width 0.08)
			)
		)
	)
	(pad "11" smd custom
		(at 1.3875 0.8)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4225 -0.06)
					(xy 0.4225 -0.06)
					(xy 0.4225 0.06)
					(xy -0.325931 0.06)
					(xy -0.4225 -0.036569)
				)
				(width 0.08)
			)
		)
	)
	(pad "12" smd roundrect
		(at 1.3875 0.4)
		(size 0.925 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.3875 0)
		(size 0.925 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.3875 -0.4)
		(size 0.925 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd custom
		(at 1.3875 -0.8)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4225 0.036569)
					(xy -0.325931 -0.06)
					(xy 0.4225 -0.06)
					(xy 0.4225 0.06)
					(xy -0.4225 0.06)
				)
				(width 0.08)
			)
		)
	)
	(pad "16" smd custom
		(at 0.8 -1.3875)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.06 -0.4225)
					(xy 0.06 -0.4225)
					(xy 0.06 0.325931)
					(xy -0.036569 0.4225)
					(xy -0.06 0.4225)
				)
				(width 0.08)
			)
		)
	)
	(pad "17" smd roundrect
		(at 0.4 -1.3875)
		(size 0.2 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 0 -1.3875)
		(size 0.2 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -0.4 -1.3875)
		(size 0.2 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd custom
		(at -0.8 -1.3875)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.06 -0.4225)
					(xy 0.06 -0.4225)
					(xy 0.06 0.4225)
					(xy 0.036569 0.4225)
					(xy -0.06 0.325931)
				)
				(width 0.08)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UQFN-20_3x3mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
