(footprint "VDFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.7mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-Lead Very Thin Dual Flatpack No-Lead (LZ) - 2x3x0.9 mm Body [VDFN] (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "DFN 0.5")
	(property "Reference" "REF**"
		(at 0 -2.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "VDFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.7mm"
		(at 0 2.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at 0 -0.425)
		(size 0.72 0.69)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0.425)
		(size 0.72 0.69)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1 -0.75)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1 -0.25)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1 0.25)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1 0.75)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1 0.75)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1 0.25)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1 -0.25)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1 -0.75)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VDFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
