(footprint "VQFN-12-1EP_4x4mm_P0.8mm_EP2.1x2.1mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "VQFN, 12 Pin (https://www.mouser.ch/datasheet/2/268/EMC2301_2_3_5_Data_Sheet_DS20006532A-3443118.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "VQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-12-1EP_4x4mm_P0.8mm_EP2.1x2.1mm"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.525 -0.525)
		(size 0.85 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.525 0.525)
		(size 0.85 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.525 -0.525)
		(size 0.85 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.525 0.525)
		(size 0.85 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.8875 -0.8)
		(size 0.925 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.8875 0)
		(size 0.925 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.8875 0.8)
		(size 0.925 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -0.8 1.8875)
		(size 0.3 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0 1.8875)
		(size 0.3 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.8 1.8875)
		(size 0.3 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1.8875 0.8)
		(size 0.925 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.8875 0)
		(size 0.925 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.8875 -0.8)
		(size 0.925 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0.8 -1.8875)
		(size 0.3 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 -1.8875)
		(size 0.3 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -0.8 -1.8875)
		(size 0.3 0.925)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd rect
		(at 0 0)
		(size 2.1 2.1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-12-1EP_4x4mm_P0.8mm_EP2.1x2.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
