(footprint "VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "VQFN, 16 Pin (https://ww1.microchip.com/downloads/en/DeviceDoc/16L_VQFN-WFS_3x3mm_4MX_C04-00508a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "VQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm_ThermalVias"
		(at 0 2.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -0.275 -0.275)
		(size 0.203785 0.203785)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.169451 -0.169451)
					(xy 0.169451 -0.169451)
					(xy 0.169451 -0.138837)
					(xy -0.138837 0.169451)
					(xy -0.169451 0.169451)
				)
				(width 0.104523)
			)
		)
	)
	(pad "" smd custom
		(at -0.275 0.275)
		(size 0.203785 0.203785)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.169451 -0.169451)
					(xy -0.138837 -0.169451)
					(xy 0.169451 0.138837)
					(xy 0.169451 0.169451)
					(xy -0.169451 0.169451)
				)
				(width 0.104523)
			)
		)
	)
	(pad "" smd custom
		(at 0.275 -0.275)
		(size 0.203785 0.203785)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.169451 -0.169451)
					(xy 0.169451 -0.169451)
					(xy 0.169451 0.169451)
					(xy 0.138837 0.169451)
					(xy -0.169451 -0.138837)
				)
				(width 0.104523)
			)
		)
	)
	(pad "" smd custom
		(at 0.275 0.275)
		(size 0.203785 0.203785)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.169451 0.138837)
					(xy 0.138837 -0.169451)
					(xy 0.169451 -0.169451)
					(xy 0.169451 0.169451)
					(xy -0.169451 0.169451)
				)
				(width 0.104523)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.4625 -0.75)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.4625 -0.25)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.4625 0.25)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.4625 0.75)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.75 1.4625)
		(size 0.25 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -0.25 1.4625)
		(size 0.25 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.25 1.4625)
		(size 0.25 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.75 1.4625)
		(size 0.25 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.4625 0.75)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.4625 0.25)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.4625 -0.25)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.4625 -0.75)
		(size 0.775 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.75 -1.4625)
		(size 0.25 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.25 -1.4625)
		(size 0.25 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -0.25 -1.4625)
		(size 0.25 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -0.75 -1.4625)
		(size 0.25 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" thru_hole circle
		(at 0 0)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" smd rect
		(at 0 0)
		(size 0.63 0.63)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "17" smd rect
		(at 0 0)
		(size 1.1 1.1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
