(footprint "Vishay_PowerPAK_MLP44-24L_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PowerPAK PowerPAK MLP44-24L (https://www.vishay.com/docs/78231/mlp44-24l.pdf)")
	(tags "powerpak mlp44-24l")
	(property "Reference" "REF**"
		(at 0 -3.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Vishay_PowerPAK_MLP44-24L_ThermalVias"
		(at 0 3.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(net_tie_pad_groups "1,2,26" "3,4,27" "5,6,7,8,9")
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.9375 -0.825 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.9375 -0.375 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.9375 0.525 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.9375 0.975 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at -1.475 1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.15 -0.2875) (xy -0.144291 -0.316201) (xy -0.128033 -0.340533) (xy -0.103701 -0.356791) (xy -0.075 -0.3625)
					(xy 0.075 -0.3625) (xy 0.103701 -0.356791) (xy 0.128033 -0.340533) (xy 0.144291 -0.316201) (xy 0.15 -0.2875)
					(xy 0.15 0.2875) (xy 0.144291 0.316201) (xy 0.128033 0.340533) (xy 0.103701 0.356791) (xy 0.075 0.3625)
					(xy -0.075 0.3625) (xy -0.103701 0.356791) (xy -0.128033 0.340533) (xy -0.144291 0.316201) (xy -0.15 0.2875)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.15 -0.3625) (xy 2.2 -0.3625) (xy 2.2 -0.0875) (xy -0.15 -0.0875)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "6" smd roundrect
		(at -1.025 1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -0.575 1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.125 1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.575 1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.025 1.935)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.9375 1.425 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.9375 0.975 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.9375 0.525 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.9375 0.075 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.9375 -0.375 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1.9375 -0.825 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.9375 -1.275 90)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.475 -1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.025 -1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 0.575 -1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 0.125 -1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -0.575 -1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -1.025 -1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -1.475 -1.9375)
		(size 0.3 0.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd rect
		(at 0.4875 -0.75 180)
		(size 1.575 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" thru_hole circle
		(at 0.49 -0.76)
		(size 0.45 0.45)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "26" smd rect
		(at -1.175 -0.75 180)
		(size 1.15 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" thru_hole circle
		(at -1.155 -0.75)
		(size 0.45 0.45)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at -1.5 0.3)
		(size 0.45 0.45)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at -1.5 1.05)
		(size 0.45 0.45)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "27" smd custom
		(at -0.75 0.775)
		(size 1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1 0.5) (xy -1 -0.7) (xy 1.825 -0.7) (xy 1.825 -0.245) (xy 1.175 -0.245) (xy 1.175 0.5)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "27" thru_hole circle
		(at -0.35 0.3)
		(size 0.45 0.45)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at -0.35 1.05)
		(size 0.45 0.45)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at 0.8 0.3)
		(size 0.45 0.45)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "28" smd roundrect
		(at 0.985 0.99 180)
		(size 0.58 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Vishay_PowerPAK_MLP44-24L.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
