(footprint "W-PDFN-8-1EP_6x5mm_P1.27mm_EP3x3mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "W-PDFN, 8 Pin (https://media-www.micron.com/-/media/client/global/documents/products/data-sheet/nor-flash/serial-nor/mt25q/die-rev-a/mt25q_qljs_u_256_aba_0.pdf#page=22), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "W-PDFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "W-PDFN-8-1EP_6x5mm_P1.27mm_EP3x3mm"
		(at 0 3.45 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.75 -0.75)
		(size 1.21 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.206612)
	)
	(pad "" smd roundrect
		(at -0.75 0.75)
		(size 1.21 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.206612)
	)
	(pad "" smd roundrect
		(at 0.75 -0.75)
		(size 1.21 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.206612)
	)
	(pad "" smd roundrect
		(at 0.75 0.75)
		(size 1.21 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.206612)
	)
	(pad "1" smd roundrect
		(at -2.85 -1.905)
		(size 1.05 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.85 -0.635)
		(size 1.05 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.85 0.635)
		(size 1.05 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.85 1.905)
		(size 1.05 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.85 1.905)
		(size 1.05 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.85 0.635)
		(size 1.05 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.85 -0.635)
		(size 1.05 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.85 -1.905)
		(size 1.05 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 3 3)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/W-PDFN-8-1EP_6x5mm_P1.27mm_EP3x3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
